For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Turn the ignition OFF.
2. Relieve the fuel system pressure. Refer to LINK.
3. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.

1 | Fuel Pressure Sensor Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Disconnect the electrical connector.

Tighten
X N·m (X lb in)