For 1990-2009 cars

#### Special Tools

EN 49411 Torque Angle Sensor Kit

For equivalent regional tools, refer to Special Tools.

1. Ensure the cylinder head locating pins are securely mounted in the cylinder block deck face.

Install a NEW cylinder head gasket bank 1 using the deck face locating pins for retention.

2. Align the cylinder head bank 1 with the deck face locating pins.
3. Place the cylinder head bank 1 in position on the deck face.

Note:

• | DO NOT allow oil on the cylinder head bolt bosses.

• | DO NOT reuse the old cylinder head bolts.

4. Install NEW 8 cylinder head bolts.

Caution: Refer to Fastener Caution in the Preface section.

5. Tighten the NEW 8 cylinder head bolts:

5.1. | Tighten first pass in sequence to 45 N·m (33 lb ft).

5.2. | Tighten second pass in sequence to an additional 120 degrees using the EN 49411 angle sensor .