For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the inside rearview mirror mount plate cover. Refer to Inside Rearview Mirror Mount Plate Cover Replacement

1 | Windshield Outside Moisture and Headlamp Automatic Control Ambient Light Sensor Retainer Tip Use a small flat-bladed tool to release the locking retainer on the windshield outside moisture and headlamp automatic control ambient light sensor and push the cap upwards.
2 | Windshield Outside Moisture and Headlamp Automatic Control Ambient Light Sensor