For 1990-2009 cars

The following service procedures require either a programming or a setup event performed for a complete repair.

### Liftgate Control Module Replacement

If the liftgate control module is replaced, the following procedures must be performed.

• | Liftgate Module Programming. Refer to Service Programming System (SPS).

• | Liftgate Calibration. Refer to Liftgate Calibration Procedure.

### Liftgate Control Module Reprogramming

Do not reprogram the liftgate control module unless directed by a service procedure or a service bulletin.

If the liftgate control module needs to be reprogrammed, refer to Service Programming System (SPS).

### Liftgate Calibration

If any portion of the power liftgate assembly is replaced, repaired or disassembled, perform the liftgate calibration procedure. Refer to Liftgate Calibration Procedure.