For 1990-2009 cars

## Mode Control Cam Actuator Replacement Left Hand Drive

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the instrument panel lower trim panel - left side. Refer to Instrument Panel Lower Trim Panel Replacement - Left Side.
3. Remove the floor air outlet duct - left side. Refer to Floor Air Outlet Duct Replacement - Left Side.

1 | Mode Actuator Fastener (Qty: 2)

#### Procedure

Disconnect the mode actuator electrical connector.

2 | Mode Actuator Tip Actuator is self-calibrating when connecting the battery.