For 1990-2009 cars

1. Remove the engine oil cooler coolant outlet hose clamps (1, 2).
2. Remove the engine oil cooler coolant outlet hose (3) and the snap lock (4).
3. Remove the engine oil cooler coolant inlet hose clamps (1).
4. Remove the engine oil cooler coolant inlet hose (2).
5. Remove the oil filter adapter bolts (2) from engine block.
6. Remove the oil filter adapter (1).
7. Remove and discard the oil filter adapter gasket.