For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the engine cover. Refer to Engine Cover Replacement
2. Remove the exhaust manifold heat shield. Refer to Exhaust Manifold Heat Shield Replacement

1 | Turbocharger Oil Feed Pipe Fastener (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 30 N·m (22 lb ft)
2 | Turbocharger Oil Feed Pipe

#### Procedure

Discard the and install a NEW turbocharger oil feed pipe gaskets prior to installation of the pipe.