For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Folder the back on left side of the backseat.
2. Lift the front left side of the luggage compartment trim floor panel and also the damping material.

1 | Electronic Suspension Rear Position Sensor Replacement Fastener (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 6 N·m(53 lb in)
2 | Electronic Suspension Rear Position Sensor