For 1990-2009 cars

For description see Trim Height Inspection, refer to Trim Height Inspection.

Z Trim Height
Suspension | Service Preferred | Tolerance
--- | --- | ---
Standard | 409-414 mm (16.1-16.3 in) | ±10 mm (0.4 in)
Sport | 397-404 mm (15.6-15.9 in) | ±10 mm (0.4 in)
AWD | 420-426 mm (16.5-16.8 in) | ±10 mm (0.4 in)
AWD Sport | 408-415 mm (16.1-16.3 in) | ±10 mm (0.4 in)
Condition: Full tank, no passengers and placed on plane ground.