For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the 2 center clips on the lower part of the rear bumper. Refer to Rear Bumper Fascia Extension Replacement.

1 | Tire Pressure Indicator Receiver Fastener (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 4 N·m (35 lb in)
2 | Tire Pressure Indicator Receiver

#### Procedure

1. Disconnect any electrical connectors as needed.
2. After repairs, program the tire pressure monitoring system. Refer to Control Module References.