For 1990-2009 cars

## Fuel Feed Pipe Replacement Plastic

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove engine appearance cover replacement. Refer to LINK.

1 | Fuel Feed Pipe Retainer (Qty: 4) Warning: Relieve the fuel system pressure before servicing fuel system components in order to reduce the risk of fire and personal injury. After relieving the system pressure, a small amount of fuel may be released when servicing the fuel lines or connections. In order to reduce the chance of personal injury, cover the regulator and the fuel line fittings with a shop towel before disconnecting. This will catch any fuel that may leak out. Place the towel in an approved container when the disconnection is complete.
2 | Fuel Feed Pipe

#### Procedure

Open the first retainer with XXXXX pipe remover and the second retainer with a small screwdriver.

#### Special Tool

XXXXX Pipe Remover

## Fuel Feed Pipe Replacement Metal

### Special Tools

EN-796-A Remover

GE-6600-207 Installer

GE-611 Torque Wrench

For equivalent regional tools, refer to Special Tools.

### Removal Procedure

1. Remove engine appearance cover replacement. Refer to XXX.
2. Remove the fastener (1) from the fuel pump module (2) with EN-796-A remover .
3. Remove the fuel feed pipe plastic (3) with EN-796-A remover from the fuel feed pipe metal (4).
4. Remove the 2 fasteners (1) and get out the fuel feed pipe metal (2).

### Installation Procedure

1. Install the 2 fasteners (1) to the intake manifold but do not tighten yet.
2. Install the fastener (2) to the fuel pump module and tighten to X N·m (X lb ft) with GE-6600-207 installer and GE-611 torque wrench .
3. Tighten the 2 fasteners (1) to X N·m (X lb ft).
4. Install the fuel feed pipe plastic to the fuel feed pipe metal.

## Fuel Feed Pipe Replacement Branch

Callout | Component Name
--- | ---
1 | Evaporative Emission Front Pipe Retainer
2 | Evaporative Emission Front Pipe

## Fuel Feed Pipe Replacement Runback

Callout | Component Name
--- | ---
1 | Evaporative Emission Front Pipe Retainer
2 | Evaporative Emission Front Pipe
3 | Evaporative Emission Front Pipe