For 1990-2009 cars

## Tail Lamp Pocket Replacement 69 NB

### Removal Procedure

1. Remove the body side outer panel. Refer to Body Side Outer Panel Replacement.

Note: Do not damage any inner panels or reinforcements.

2. Cut out the tail lamp pocket roughly.

Note: Note the number and location of the welds for installations of the service part.

3. Locate and drill out all of the necessary factory welds.
4. Remove the damaged tail lamp pocket.

### Installation Procedure

1. Prepare new tail lamp pocket in the area (1).

3x slots 8x24 mm (0.3x0.9 in).

2. Prepare all attachment surfaces as necessary.
3. Apply bodywork repair through structural adhesive to body. Refer to Structural Adhesive Body Repairs.
4. Position the tail lamp pocket.

Note: Refer to Welded, Brazed, and Riveted Joint Specifications.

5. Spot weld the tail lamp pocket accordingly.
6. MIG-braze the tail lamp pocket.
7. Grind MIG-brazed seams.
8. Apply the sealers and anti-corrosion materials to the repair area, as necessary. Refer to Anti-Corrosion Treatment and Repair.
9. Install the body side outer panel. Refer to Body Side Outer Panel Replacement.