For 1990-2009 cars

## Water Pump Replacement LBW/A28NET

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the drive belt. Refer to Drive Belt Replacement.
2. Drain the cooling system. Refer to Cooling System Draining and Filling.

1 | Water Pump

#### Procedure

1. Remove the water pump. Refer to Water Pump Removal.
2. Install the water pump. Refer to Water Pump Installation.

## Water Pump Replacement LDE/A16XER, 2H0/A18XER

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement.
2. Remove the drive belt. Refer to Drive Belt Replacement.
3. Remove the water pump pulley. Refer to Water Pump Pulley Replacement.
4. Drain the coolant. Refer to Cooling System Draining and Filling.

1 | Water Pump Fastener (Qty: 5) Caution: Refer to Fastener Caution in the Preface section. Tighten 8 N·m (71 lb in)
2 | Water Pump