For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the water deflector. Refer to Front Side Door Water Deflector Replacement.
2. Move the window to the full up position.
3. Remove check link cover.

1 | Front Side Door Check Link Fastener (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
2 | Front Side Door Check Link Assembly

#### Procedure

Remove the check link from the inside of the door.