For 1990-2009 cars

## Duct Air Temperature Sensor Replacement - Lower Left Side Left Hand Drive

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the instrument panel lower trim panel - driver side. Refer to Instrument Panel Lower Trim Panel Replacement - Left Side.
2. Remove the floor air outlet duct - left side. Refer to Floor Air Outlet Duct Replacement - Left Side.

1 | Air Temperature Sensor - Lower Left Side

#### Procedure

1. Disconnect the air temperature sensor electrical connector.
2. Twist and pull the lower air temperature sensor from the HVAC module assembly.