For 1990-2009 cars

#### Special Tools

EN 47631 Crankshaft Position Sensor Bolt

For equivalent regional tools, refer to Special Tools.

1. Install the crankshaft position sensor.
2. Install the crankshaft position sensor bolt (1).
3. Install the EN 47631 bolt

Caution: Refer to Fastener Caution in the Preface section.

4. Install the crankshaft position sensor bolt (1) and tighten to 10 N·m (89 lb in).