For 1990-2009 cars

1. Measure the alignment on an alignment rack. Refer to Wheel Alignment Measurement.

Note: Do not tighten the new fasteners yet in order to allow for movement.

2. Rotate the cam nut in order to adjust the toe angle. Refer to Wheel Alignment Specifications.
3. Hand tighten the cam bolt, but do not tighten the bolt to the specification yet.
4. Reinspect the rear toe angle and adjust as necessary.

Caution: Refer to Fastener Caution in the Preface section.

5. Hold the cam nut and tighten the cam bolt.

Tighten
150 N·m (111 lb ft)

6. Repeat the procedure for the other rear wheel.
7. Lower the vehicle.