For 1990-2009 cars

#### Special Tools

• | EN 956-1 Extension

• | EN 6347 Holder

For equivalent regional tools, refer to Special Tools.

1. Install the fuel injection pump driven sprocket (2) in the correct position (1).
2. Install the fuel injection pump driven sprocket nut (3).
3. Install the EN 6347 holder (1) with EN 956-1 extension (2) to the fuel injection pump driven sprocket.

Caution: Refer to Fastener Caution in the Preface section.

4. Tighten the fuel injection pump driven sprocket nut to XX N·m (XX lb ft).
5. Remove the EN 6347 holder with EN 956-1 extension from the fuel injection pump driven sprocket.