For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Clutch Pedal Cruise Control Release Switch Fastener Caution: Refer to Fastener Caution in the Preface section. Tighten 3 N·m(26.5 lb in)
2 | Clutch Pedal Cruise Control Release Switch

#### Procedure

1. Disconnect the electrical connector.
2. Rotate the clutch pedal cruise control release switch counterclockwise to release from retaining dowel.
3. Remove the clutch pedal cruise control release switch.
4. Calibrate the brake pedal position sensor. Refer to Brake Pedal Position Sensor Calibration.