For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove engine appearance cover replacement. Refer to XXX.
2. Remove the charge air cooler inlet air tube. Refer to XXX.
3. Remove the fuel pump cover. Refer to XXX.

1 | Fuel Feed Intermediate Pipe Fastener (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten X N·m (X lb ft)
2 | Fuel Feed Intermediate Pipe