For 1990-2009 cars

This master DTC list includes all applicable DTCs in alphanumeric order with descriptors.

DTC | DTC Descriptor | Module That Sets the DTC | Diagnostic Procedure
--- | --- | --- | ---
B0000 | Vehicle Speed Information Circuit | Radio | DTC B0000
B0012 | Driver Frontal Deployment Loop Stage 1 | SDM | DTC B0012 or B0013
B0013 | Driver Frontal Deployment Loop Stage 2 | SDM | DTC B0012 or B0013
B0014 | Driver Side Deployment Loop | SDM | DTC B0014-B0045
B0015 | Driver Seat Belt Pretensioner Deployment Loop | SDM | DTC B0014-B0045
B0016 | Left Roof Rail Deployment Loop Stage 1 | SDM | DTC B0014-B0045
B0018 | Left Roof Rail Deployment Loop Stage 2 | SDM | DTC B0014-B0045
B0019 | Passenger Frontal Deployment Loop Stage 1 | SDM | DTC B0014-B0045
B001A | Driver Seat Belt Pretensioner Deployment Loop 2 | SDM | DTC B001A
B001B | Passenger Seat Belt Pretensioner Deployment Loop 2 | SDM | DTC B001B
B0020 | Passenger Frontal Deployment Loop Stage 2 | SDM | DTC B0014-B0045
B0021 | Passenger Side Deployment Loop | SDM | DTC B0014-B0045
B0022 | Passenger Seat Belt Pretensioner Deployment Loop | SDM | DTC B0014-B0045
B0023 | Right Roof Rail Deployment Loop Stage 1 | SDM | DTC B0014-B0045
B0025 | Right Roof Rail Deployment Loop Stage 2 | SDM | DTC B0014-B0045
B0051 | Deployment Commanded | SDM | DTC B0051
B0052 | Deployment Commanded | SDM | DTC B0052
B0072 | Left Front Seat Belt Sensor Circuit | SDM | DTC B0072
B0073 | Right Front Seat Belt Sensor Circuit | SDM | DTC B0073
B0074 | Passenger Occupant Classification Sensor Circuit | SDM | DTC B0074
B0075 | Left Rear Seat Belt Sensor Circuit | SDM | DTC B0075
B0076 | Right Rear Seat Belt Sensor Circuit | SDM | DTC B0076
B0077 | Center Rear Seat Belt Sensor Circuit | SDM | DTC B0077
B0081 | Passenger Presence System Malfunction | SDM | DTC B0081
B0083 | Front Impact Sensor 1 | SDM | DTC B0083-B0088
B0084 | Front Impact Sensor 2 | SDM | DTC B0083-B0088
B0085 | Left Front Side Impact Sensor | SDM | DTC B0083-B0088
B0086 | Right Front Side Impact Sensor | SDM | DTC B0083-B0088
B0087 | Left Rear Side Impact Sensor | SDM | DTC B0083-B0088
B0088 | Right Rear Side Impact Sensor | SDM | DTC B0083-B0088
B0158 | Outside Air Temperature Sensor Circuit | Instrument Cluster | DTC B0158
B0163 | Passenger Compartment Temperature Sensor Circuit | Heater and Blower and Air Conditioning Control Module | DTC B0163, B0183, or B1405
B0173 | Upper Left Outlet Air Temperature Sensor Circuit | Heater and Blower and Air Conditioning Control Module | DTC B0173, B0178, B0509, B0514 or B3933
B0178 | Lower Left Outlet Air Temperature Sensor Circuit | Heater and Blower and Air Conditioning Control Module | DTC B0173, B0178, B0509, B0514 or B3933
B0183 | Solar Load Sensor Circuit | Heater and Blower and Air Conditioning Control Module | DTC B0163, B0183, or B1405
B018A | Windshield Temperature Sensor Circuit | Heater and Blower and Air Conditioning Control Module | DTC B018A, B048C, B048F, or B1395
B0193 | Front Blower Motor Speed Circuit | Heater and Blower and Air Conditioning Control Module | DTC B0193 with CJ2 or C68 or DTC B0193 with C67
B0223 | Recirculate Position Command 1 Circuit | Heater and Blower and Air Conditioning Control Module | DTC B0223, B022A, B0233, B023A, B0408, or B0418 with CJ2 or C68 or DTC B0223, B0233, B023A, or B0408 with C67
B022A | Recirculate Position Command 2 Circuit | Heater and Blower and Air Conditioning Control Module | DTC B0223, B022A, B0233, B023A, B0408, or B0418
B0233 | Air Flow Control Circuit | Heater and Blower and Air Conditioning Control Module | DTC B0223, B022A, B0233, B023A, B0408, or B0418 with CJ2 or C68 or DTC B0223, B0233, B023A, or B0408 with C67
B023A | HVAC Actuators Supply Voltage | Heater and Blower and Air Conditioning Control Module | DTC B0223, B022A, B0233, B023A, B0408, or B0418 with CJ2 or C68 or DTC B0223, B0233, B023A, or B0408 with C67
B0283 | Rear Defrost Circuit | Heater and Blower and Air Conditioning Control Module | DTC B0283
B0408 | Main Temperature Control Circuit | Heater and Blower and Air Conditioning Control Module | DTC B0223, B022A, B0233, B023A, B0408, or B0418 with CJ2 or C68 or DTC B0223, B0233, B023A, or B0408 with C67
B0418 | Right Temperature Control Circuit | Heater and Blower and Air Conditioning Control Module | DTC B0223, B022A, B0233, B023A, B0408, or B0418
B048C | Humidity Sensor Humidity Circuit | Heater and Blower and Air Conditioning Control Module | DTC B018A, B048C, B048F, or B1395
B048D | Auxiliary Heater Temperature Command Circuit | Heater and Blower and Air Conditioning Control Module | DTC B048D or B048E with CJ2 or C68 or DTC B048D or B048E with C67
B048E | Auxiliary Heater System Malfunction | Heater and Blower and Air Conditioning Control Module | DTC B048D or B048E with CJ2 or C68 or DTC B048D or B048E with C67
B048C | Humidity Sensor Humidity Circuit | Heater and Blower and Air Conditioning Control Module | DTC B018A, B048C, B048F, or B1395
B048F | Humidity Sensor Temperature Circuit | Heater and Blower and Air Conditioning Control Module | DTC B018A, B048C, B048F, or B1395
B0509 | Upper Right Outlet Air Temperature Sensor Circuit | Heater and Blower and Air Conditioning Control Module | DTC B0173, B0178, B0509, B0514 or B3933
B0514 | Lower Right Outlet Air Temperature Sensor Circuit | Heater and Blower and Air Conditioning Control Module | DTC B0173, B0178, B0509, B0514 or B3933
B0550 | Odometer Circuit | BCM | DTC B0550
B0655 | Brake Lamp Switch Circuit | BCM | DTC B0655
B0685 | Security System Indicator Circuit | BCM | DTC B0685
B071F | Remote PRNDL Indicator | BCM | DTC B071F
B0954 | Parking Aid Front Sensor Left Corner Circuit | Object Alarm Module | DTC B0954, B0955, B0956, or B0957
B0955 | Parking Aid Front Sensor Left Middle Circuit | Object Alarm Module | DTC B0954, B0955, B0956, or B0957
B0956 | Parking Aid Front Sensor Right Middle Circuit | Object Alarm Module | DTC B0954, B0955, B0956, or B0957
B0957 | Parking Aid Front Sensor Right Corner Circuit | Object Alarm Module | DTC B0954, B0955, B0956, or B0957
B0958 | Parking Aid Rear Sensor Left Corner Circuit | Object Alarm Module | DTC B0958, B0959, B0960, or B0961
B0959 | Parking Aid Rear Sensor Left Middle Circuit | Object Alarm Module | DTC B0958, B0959, B0960, or B0961
B0960 | Parking Aid Rear Sensor Right Middle Circuit | Object Alarm Module | DTC B0958, B0959, B0960, or B0961
B0961 | Parking Aid Rear Sensor Right Corner Circuit | Object Alarm Module | DTC B0958, B0959, B0960, or B0961
B0967 | Parking Aid On/Off Switch Circuit | Object Alarm Module | DTC B0967 or B0968
B0968 | Parking Aid On/Off Switch Indicator Circuit | Object Alarm Module | DTC B0967 or B0968
B096B | Parking Aid Switch Parallel Parking Circuit | Object Alarm Module | DTC B096B
B096C | Parking Aid Side Sensor Left Front Circuit | Object Alarm Module | DTC B096C or B096D
B096D | Parking Aid Side Sensor Right Front Circuit | Object Alarm Module | DTC B096C or B096D
B0980 | Transmission Shift Pattern Selector Switch 1 Circuit | BCM | DTC B0980
B0982 | Transmission Shift Pattern Selector Switch 2 Circuit | BCM | DTC B0982
B0984 | Left Headlamp Light Distribution Shutter Control Circuit | Headlamp Control Module | DTC B0984 or B0985
B0985 | Right Headlamp Light Distribution Shutter Control Circuit | Headlamp Control Module | DTC B0984 or B0985
B1000 | Electronic Control Unit | -- | DTC B1000
B1001 | Option Configuration | -- | DTC B1001
SDM | DTC B1001
B1015 | Vehicle Identification Number Information Error | Object Alarm Module | DTC B1015
B1019 | System Configuration Error | SDM | DTC B1019
B101D | ECU Hardware | -- | DTC B101D
SDM | DTC B101D
B101E | ECU Software | -- | DTC B101E
SDM | DTC B101E
B1020 | Auxiliary Electronic Control Unit Performance | Radio | DTC B1020
B1025 | Left Front Audio Output Circuit | Radio | DTC B1025, B1035, B1045, or B1055
B1035 | Right Front Audio Output Circuit | Radio | DTC B1025, B1035, B1045, or B1055
B1045 | Left Rear Audio Output Circuit | Radio | DTC B1025, B1035, B1045, or B1055
B1055 | Right Rear Audio Output Circuit | Radio | DTC B1025, B1035, B1045, or B1055
B1259 | Antenna Ground Circuit | Digital Audio Broadcast Receiver | DTC B1259
B1271 | Theft Protection Active | Radio | DTC B1271
B1278 | Left Auxiliary Input Signal Circuit | Radio | DTC B1278 or B1279
B1279 | Right Auxiliary Input Signal Circuit | Radio | DTC B1278 or B1279
B1287 | Amplifier Control Signal Circuit | Radio | DTC B1287
B1325 | Control Module Power Circuit | -- | DTC B1325
B1370 | Control Module Ignition On and Start Circuit | BCM | DTC B1370-B1379, B1380-B1389, or B1440-B1443
B1380 | Control Module Ignition Accessory Circuit | BCM | DTC B1370-B1379, B1380-B1389, or B1440-B1443
B138A | Control Module Voltage Reference Output Circuit | Object Alarm Module | DTC B138A
B1395 | Control Module Voltage Reference Output Circuit | Heater and Blower and Air Conditioning Control Module | DTC B018A, B048C, B048F, or B1395 with CJ2 or C68
B1405 | Control Module Voltage Reference Output 2 Circuit | BCM | DTC B1405
Heater and Blower and Air Conditioning Control Module | DTC B0163, B0183, or B1405 with CJ2 or C68
Memory Seat Module | DTC B1405
B1441 | Control Module Ignition Off, Run, and Start Circuit | BCM | DTC B1370-B1379, B1380-B1389, or B1440-B1443
B1445 | Control Module Voltage Output Circuit | BCM | DTC B1445
B144A | RUN Power Relay Circuit | BCM | DTC B144A
B144B | Run/Start Power Relay Circuit | BCM | DTC B144B
B1461 | Left Headlamp Horizontal Motor Circuit | Headlamp Control Module | DTC B1461 or B1462
B1462 | Right Headlamp Horizontal Motor Circuit | Headlamp Control Module | DTC B1461 or B1462
B147E | Logistics Mode Relay Set Secondary Circuit | BCM | DTC B147E
B147F | Logistics Mode Relay Reset Secondary Circuit | BCM | DTC B147F
B1516 | Battery Current Sensor | BCM | DTC B1516
B1517 | Battery Voltage | BCM | DTC B1517
B1527 | High Parasitic Load Detected | BCM | DTC B1527
B1529 | Control Module Voltage Reference Output 5 Circuit | BCM | DTC B1529
B154A | Driver Mirror | Outside Mirror Switch | DTC B154A or B154B
B154B | Passenger Mirror | Passenger Window Switch | DTC B154A or B154B
B1735 | Seat Front Up Switch Circuit | Memory Seat Module | DTC B1735, B1740, B1745, B1750, B1755, B1760, B1815, or B1820
B1740 | Seat Front Down Switch Circuit | Memory Seat Module | DTC B1735, B1740, B1745, B1750, B1755, B1760, B1815, or B1820
B1745 | Seat Rear Up Switch Circuit | Memory Seat Module | DTC B1735, B1740, B1745, B1750, B1755, B1760, B1815, or B1820
B1750 | Seat Rear Down Switch Circuit | Memory Seat Module | DTC B1735, B1740, B1745, B1750, B1755, B1760, B1815, or B1820
B1755 | Seat Assembly Forward Switch Circuit | Memory Seat Module | DTC B1735, B1740, B1745, B1750, B1755, B1760, B1815, or B1820
B1760 | Seat Assembly Rearward Switch Circuit | Memory Seat Module | DTC B1735, B1740, B1745, B1750, B1755, B1760, B1815, or B1820
B1815 | Seat Recline Forward Switch Circuit | Memory Seat Module | DTC B1735, B1740, B1745, B1750, B1755, B1760, B1815, or B1820
B1820 | Seat Recline Rearward Switch Circuit | Memory Seat Module | DTC B1735, B1740, B1745, B1750, B1755, B1760, B1815, or B1820
B1825 | Driver Seat Recline Position Sensor Circuit | Memory Seat Module | DTC B1825, B2355, B2365, or B2375
B1925 | Left Seat Cushion Heater Sensor Circuit | Heated Seat Module, Memory Seat Module | DTC B1925 or B2170
B2170 | Right Seat Cushion Heater Sensor Circuit | Heated Seat Module, Memory Seat Module | DTC B1925 or B2170
B2355 | Driver Seat Front Vertical Position Sensor Circuit | Memory Seat Module | DTC B1825, B2355, B2365, or B2375
B2365 | Driver Seat Rear Vertical Position Sensor Circuit | Memory Seat Module | DTC B1825, B2355, B2365, or B2375
B2375 | Driver Seat Assembly Horizontal Position Sensor Circuit | Memory Seat Module | DTC B1825, B2355, B2365, or B2375
B2425 | Left Seat Cushion Heater Circuit | Heated Seat Module, Memory Seat Module | DTC B2425 or B2430
B242A | Seat Heaters Common Circuit | Heated Seat Module, Memory Seat Module | DTC B242A
B2430 | Right Seat Cushion Heater Circuit | Heated Seat Module, Memory Seat Module | DTC B2425 or B2430
B2462 | Global Positioning System Signal | Radio | DTC B2462
B2485 | Wireless Communication Antenna Circuit | Mobile Telephone Control Module | DTC B2485
B2530 | Front Fog Lamps Control Circuit | BCM | DTC B2530
B2540 | Rear Fog Lamps Control Circuit | BCM | DTC B2540
B2545 | Backup Lamps Control Circuit | BCM | DTC B2545
B255D | Passenger Compartment Lamp Color 2 Control Circuit | BCM | DTC B255D
B257A | Headlamp Switch Input Signals Correlation | BCM | DTC B257A
B257B | Lighting Control Switch Signal | BCM | DTC B257B
B2580 | High Beam Control Circuit | BCM | DTC B2580
B2585 | Park Lamps Control Circuit | BCM | DTC B2585 or B3867
B258A | Low Beam Control Circuit | BCM | DTC B258A
B2590 | Left Cornering Lamp Circuit | Headlamp Control Module | DTC B2590 or B2595
B2595 | Right Cornering Lamp Circuit | Headlamp Control Module | DTC B2590 or B2595
B260B | Left Daytime Running Lamp Relay Control Circuit | BCM | DTC B260B or B260C
B260C | Right Daytime Running Lamp Relay Control Circuit | BCM | DTC B260B or B260C
B2610 | Passenger Compartment Dimming 1 Circuit | BCM | DTC B2610
B2615 | Passenger Compartment Dimming 2 Circuit | BCM | DTC B2615
B2625 | Display Dimming Pulse Width Modulation Output Circuit | BCM | DTC B2625
B2645 | Ambient Light Sensor Circuit | BCM | DTC B2645
B2652 | Passenger Compartment Dimming 3 Circuit | BCM | DTC B2652
B270A | Park Lock Solenoid Actuator Control Circuit | BCM | DTC B270A
B2740 | Front Fog Lamp Switch Circuit | BCM | DTC B2740
B2750 | Horn Relay Secondary Circuit | BCM | DTC B2750
B2755 | Driver Memory Select Switch Circuit | Memory Seat Module | DTC B2755 or B2765
B2765 | Seat Memory Set Switch Circuit | Memory Seat Module | DTC B2755 or B2765
B291A | Content Theft Deterrent Assembly | BCM | DTC B291A
B291B | Content Theft Deterrent Sensor | BCM | DTC B291B
B3006 | Hood Ajar Circuit | BCM | DTC B3006
B3031 | Security Controller In Learn Mode | BCM | DTC B3031
B3055 | No Transponder Modulation or No Transponder | BCM | DTC B3055
B3060 | Unprogrammed Transponder Identification Code Received | BCM | DTC B3060
B3101 | Keyless Entry Data Link Circuit | BCM | DTC B3101
B3105 | Keyless Entry System Key Fobs Not Programmed | Remote Control Door Lock Receiver | DTC B3105
B3106 | Keyless Entry Data Link | BCM | DTC B3106
B3109 | Keyless Transmitter 1 Battery | Remote Control Door Lock Receiver | DTC B3109-B3113
B310D | Keyless Entry Transmitter 6 Battery | Remote Control Door Lock Receiver | DTC B310D-B310F
B310E | Keyless Entry Transmitter 7 Battery | Remote Control Door Lock Receiver | DTC B310D-B310F
B310F | Keyless Entry Transmitter 8 Battery | Remote Control Door Lock Receiver | DTC B310D-B310F
B3110 | Keyless Entry Transmitter 2 Battery | Remote Control Door Lock Receiver | DTC B3109-B3113
B3111 | Keyless Entry Transmitter 3 Battery | Remote Control Door Lock Receiver | DTC B3109-B3113
B3112 | Keyless Entry Transmitter 4 Battery | Remote Control Door Lock Receiver | DTC B3109-B3113
B3113 | Keyless Entry Transmitter 5 Battery | Remote Control Door Lock Receiver | DTC B3109-B3113
B3119 | Keyless Entry Antenna 1 | Remote Control Door Lock Receiver | DTC B3119
B3120 | Keyless Entry Antenna 2 | Remote Control Door Lock Receiver | DTC B3120
B3121 | Keyless Entry Antenna 3 | Remote Control Door Lock Receiver | DTC B3121
B3122 | Keyless Entry Antenna 4 | Remote Control Door Lock Receiver | DTC B3122
B2123 | Keyless Entry Antenna 5 | Remote Control Door Lock Receiver | DTC B3123
B2124 | Keyless Entry Antenna 6 | Remote Control Door Lock Receiver | DTC B3124
B3125 | Driver Door Only Unlock Circuit | BCM | DTC B3125, B3130, or B3135
B3130 | All Door Unlock Circuit | BCM | DTC B3125, B3130, or B3135
B3135 | All Door Lock Circuit | BCM | DTC B3125, B3130, or B3135
B3140 | Door Unlock Switch Circuit | BCM | DTC B3140 or B3150
B3150 | Door Lock Switch Circuit | BCM | DTC B3140 or B3150
B316B | Driver Window Switch | Window Switch | DTC B316B, B317A, B318A, or B319A
B317A | Right Front/Passenger Window Switch | Window Switch | DTC B316B, B317A, B318A, or B319A
B318A | Left Rear Window Switch | Window Switch | DTC B316B, B317A, B318A, or B319A
B319A | Right Rear Window Switch | Window Switch | DTC B316B, B317A, B318A, or B319A
B3205 | Driver Window Motor Circuit | BCM | DTC B3205, B3210, B3215, or B3220
B3210 | Passenger Window Motor Circuit | BCM | DTC B3205, B3210, B3215, or B3220
B3215 | Left Rear Window Motor Circuit | BCM | DTC B3205, B3210, B3215, or B3220
B3220 | Right Rear Window Motor Circuit | BCM | DTC B3205, B3210, B3215, or B3220
B3265 | Trunk Lid Unlatch Output Circuit | BCM | DTC B3265
B3410 | Automatic Headlamp Leveling Control Module Front Axle Sensor Signal Circuit | Headlamp Control Module | DTC B3410 or B3420
B3415 | Automatic Headlamp Leveling Control Module Front Axle Sensor Supply Circuit | Headlamp Control Module | DTC B3415
B3420 | Automatic Headlamp Leveling Control Module Rear Axle Sensor Signal Circuit | Headlamp Control Module | DTC B3410 or B3420
B3445 | Brake Lamps Circuit | BCM | DTC B3445 or B3878
B3567 | Driver Information Center Switch Circuit | Instrument Cluster | DTC B3567
B3588 | Rear Fog Lamp Switch Circuit | BCM | DTC B3588
B3596 | Hazard Lamps Request Circuit | BCM | DTC B3596
B3618 | Exterior Liftgate Unlatch Switch Circuit | BCM | DTC B3618
B3622 | Steering Wheel Controls Signal Circuit | BCM | DTC B3622
B3650 | High Beam and Headlamp Flash Select Circuit | BCM | DTC B3650
B3664 | Sunroof Position Select Switch High Signal Circuit | Sunroof Module | DTC B3664
B3697 | Sunroof Actuator Malfunction | Sunroof Module | DTC B3697
B369B | Sunroof Sunshade Position Select Switch Circuit | Sunshade Module | DTC B369B
B369C | Sunroof Ventilation Position Select Switch Circuit | Sunroof Module | DTC B369C
B369D | Sunroof Sunshade Actuator Malfunction | Sunshade Module | DTC B369D
B370A | Rain Sensor | BCM | DTC B370A
B3715 | Front Wiper Relay Circuit | BCM | DTC B3715 or B3875
B371B | Rear Wiper Function Control Circuit | BCM | DTC B370B
B3794 | Cruise Control Function Request Circuit | BCM | DTC B3794
B3797 | All Door Dead Lock Circuit | BCM | DTC B3797
B3806 | High Beam and Headlamp Flash Select Circuit | BCM | DTC B3806
B3810 | Headlamp Washer Relay Circuit | BCM | DTC B3810 or B3811
B3811 | Rear Washer Relay Circuit | BCM | DTC B3810 or B3811
B3843 | Outside Air Quality Sensor Circuit | Heater and Blower and Air Conditioning Control Module | DTC B3843 with CJ2 or C68
B3867 | Right Park Lamps Control Circuit | BCM | DTC B2585 or B3867
B3873 | Front Washer Relay Circuit | BCM | DTC B3873
B3875 | Windshield Wiper High Speed Relay Circuit | BCM | DTC B3715 or B3875
B3878 | Right Brake Lamp Circuit | BCM | DTC B3445 or B3878
B3881 | Left Tail Lamp Circuit | BCM | DTC B3881 or B3882
B3882 | Right Tail Lamp Circuit | BCM | DTC B3881 or B3882
B3883 | License Plate Lamp Circuit | BCM | DTC B3883
B3884 | Center High Mounted Brake Lamp Circuit | BCM | DTC B3884
B3885 | Trailer Left Tail Lamp Circuit | BCM | DTC B3885 or B3886
B3886 | Trailer Right Tail Lamp Circuit | BCM | DTC B3885 or B3886
B3887 | Trailer Left Turn Signal Circuit | BCM | DTC B3887 or B3888
B3888 | Trailer Right Turn Signal Circuit | BCM | DTC B3887 or B3888
B3889 | Trailer Brake Lamps Circuit | BCM | DTC B3889
B388B | Secondary Left Tail and Brake Lamp Circuit | BCM | DTC B388B or B388C
B388C | Secondary Right Tail and Brake Lamp Circuit | BCM | DTC B388B or B388C
B3890 | Trailer Backup Lamps Circuit | BCM | DTC B3890
B3891 | Trailer Fog Lamps Circuit | BCM | DTC B3891
B3902 | Incorrect Immobilizer Identifier Received | BCM | DTC B3902
B3933 | Air Conditioning Evaporator Temperature Sensor Circuit | Heater and Blower and Air Conditioning Control Module | DTC B0173, B0178, B0509, B0514 or B3933 with CJ2 or C68 or DTC B3933 with C67
B3935 | Transponder Authentication Error | BCM | DTC B3935
B3938 | Fuel Door Actuator Lock Circuit | BCM | DTC B3938
B393B | Air Conditioning Compressor Valve Control Circuit | Heater and Blower and Air Conditioning Control Module | DTC B0173, B0178, B0509, B0514 or B3933 with CJ2 or C68 or DTC B3933 with C67
B3948 | Left Front Turn Signal Circuit | BCM | DTC B3948 or B3949
B3949 | Right Front Turn Signal Circuit | BCM | DTC B3948 or B3949
B3950 | Left Rear Turn Signal Circuit | BCM | DTC B3950 or B3951
B3951 | Right Rear Turn Signal Circuit | BCM | DTC B3950 or B3951
B3976 | Unconfigured Transponder | BCM | DTC B3976
B3984 | Device 1 Environment Identifier Not Programmable | BCM | DTC B3984
C0000 | Vehicle Speed Information Circuit | EBCM | DTC C0000
C0010 | Reverse Gear Signal Circuit | ECM | DTC C0010
C0035 | Left Front Wheel Speed Sensor Circuit | EBCM | DTC C0035, C0040, C0045, or C0050
C0040 | Right Front Wheel Speed Sensor Circuit | EBCM | DTC C0035, C0040, C0045, or C0050
C0045 | Left Rear Wheel Speed Sensor Circuit | EBCM | DTC C0035, C0040, C0045, or C0050
C0050 | Right Rear Wheel Speed Sensor Circuit | EBCM | DTC C0035, C0040, C0045, or C0050
C0110 | Pump Motor Circuit | EBCM | DTC C0110
C0131 | Traction Control System Pressure Circuit | EBCM | DTC C0131
C0161 | Antilock Braking System Brake Switch Circuit | EBCM | DTC C0161
C0187 | Lateral Acceleration Sensor Circuit | EBCM | DTC C0187, C0196, C019B, C0287, or C0297
C0196 | Yaw Rate Circuit | EBCM | DTC C0187, C0196, C019B, C0287, or C0297
C019B | Yaw Rate Signal | EBCM | DTC C0187, C0196, C019B, C0287, or C0297
C0242 | Powertrain Control Module Indicated Traction Control Malfunction | ECM | DTC C0242 or P0856
C0245 | Wheel Speed Sensor Frequency Malfunction | EBCM | DTC C0245
C0252 | Vehicle Stability Control Module Sensors Correlation | EBCM | DTC C0252
C0267 | Low Brake Fluid Indicated | EBCM | DTC C0267
C0274 | Isolation Valve | EBCM | DTC C0274, C2075, or C0280
C0275 | Dump Valve | EBCM | DTC C0274, C2075, or C0280
C0277 | Brake Pedal Position Sensor Circuit | BCM | DTC C0277
C0280 | Stability System Active Too Long | EBCM | DTC C0274, C2075, or C0280
C0287 | Longitudinal Acceleration Sensor Circuit | EBCM | DTC C0187, C0196, C019B, C0287, or C0297
C028A | Park Brake Motor Circuit | Parking Brake Control Module | DTC C028A
C028B | Park Brake Motor Position Sensor Signal | Parking Brake Control Module | DTC C028B
C028D | Replace Park Brake Pad | Parking Brake Control Module | DTC C028D
C028F | Park Brake Solenoid Actuator Circuit | Parking Brake Control Module | DTC C028F
C0293 | Park Brake Switch Control | Parking Brake Control Module | DTC C0293
C0297 | Lost Communication With Yaw Rate Sensor | EBCM | DTC C0187, C0196, C019B, C0287, or C0297
C0298 | Park Brake Unlatch Switch Circuit | Parking Brake Control Module | DTC C0298
C0393 | Rear Axle Coupling Solenoid Valve Control Circuit | Rear Differential Clutch Control Module | DTC C0393
C0402 | Transfer Case Solenoid Valve | Rear Differential Clutch Control Module | DTC C0402
C0403 | Transfer Case Solenoid Valve | Rear Differential Clutch Control Module | DTC C0403
C0406 | Transfer Case Solenoid Valve Control Circuit | Rear Differential Clutch Control Module | DTC C0406
C0407 | AWD Oil Pump Motor | Rear Differential Clutch Control Module | DTC C0407
C0408 | Rear Axle Coupling Solenoid Valve | Rear Differential Clutch Control Module | DTC C0408
C0450 | Steering Assist Control Actuator Circuit | Power Steering Control Module | DTC C0450
C0460 | Steering Position | EBCM | DTC C0460 or C0710
C0550 | Electronic Control Unit | EBCM | DTC C0550
C0558 | Calibration Data | Parking Brake Control Module | DTC C028D
C0561 | System Disabled Information Stored | Parking Brake Control Module | DTC C028D
C0569 | System Configuration | BCM | DTC C0569
C056D | Electronic Control Unit Hardware | EBCM | DTC C056D
ECU Hardware Performance | Parking Brake Control Module | DTC C056D
C056E | Electronic Control Unit Software | EBCM | DTC C056E
Parking Brake Control Module | DTC C056E
C0574 | Circuit Board Temperature Sensor Sensor | Parking Brake Control Module | DTC C0574
Rear Differential Clutch Control Module | DTC C0574
C0575 | Left Front Actuator Circuit | Suspension Control Module | DTC C0575, C0580, C0585, or C0590
C0580 | Right Front Actuator Circuit | Suspension Control Module | DTC C0575, C0580, C0585, or C0590
C0585 | Left Rear Actuator Circuit | Suspension Control Module | DTC C0575, C0580, C0585, or C0590
C0590 | Right Rear Actuator Circuit | Suspension Control Module | DTC C0575, C0580, C0585, or C0590
C0595 | Left Front Acceleration Sensor Circuit | Suspension Control Module | DTC C0595, C0600, or C0605
C0600 | Right Front Acceleration Sensor Circuit | Suspension Control Module | DTC C0595, C0600, or C0605
C0605 | Left Rear Acceleration Sensor Circuit | Suspension Control Module | DTC C0595, C0600, or C0605
C0670 | Left Front Acceleration or Position Sensor Circuit | Suspension Control Module | DTC C0670 or C0675
C0675 | Right Front Acceleration or Position Sensor Circuit | Suspension Control Module | DTC C0670 or C0675
C0710 | Steering Position Signal | EBCM | DTC C0460 or C0710
C0720 | Engine Torque Management Feedback Signal | Suspension Control Module | DTC C0720
C0750 | Left Front Low Tire Pressure Sensor | BCM | DTC C0750, C0755, C0760, or C0765
C0755 | Right Front Low Tire Pressure Sensor | BCM | DTC C0750, C0755, C0760, or C0765
C0760 | Left Rear Low Tire Pressure Sensor | BCM | DTC C0750, C0755, C0760, or C0765
C0765 | Right Rear Low Tire Pressure Sensor | BCM | DTC C0750, C0755, C0760, or C0765
C0775 | Tire Pressure Monitoring System Sensors | BCM | DTC C0775
C078A | Tire Pressure Indicator Module | BCM | DTC C078A
C0800 | Control Module Power Circuit | Power Steering Control Module | DTC C0800
C0870 | Control Module Voltage Reference Output Circuit | Suspension Control Module | DTC C0870
P0008 | Engine Position System Performance Bank 1 | ECM | DTC P0008 or P0009
P0009 | Engine Position System Performance Bank 2 | ECM | DTC P0008 or P0009
P000A | Intake Camshaft Position System Performance | ECM | DTC P000A or P000B
P000B | Exhaust Camshaft Position System Performance | ECM | DTC P000A or P000B
P0010 | Intake Camshaft Position Actuator Solenoid Control Circuit | ECM | DTC P0010 or P0013 for the 1.6L (LDE) and 1.8L (2H0) engine or DTC P0010, P0013, or P2088-P2091 for the 2.0L engine
Intake Camshaft Position Actuator Solenoid Control Circuit Bank 1 | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0011 | Intake Camshaft Position System Performance | ECM | DTC P0011 or P0014 for the 1.6L (LDE) and 1.8L (2H0) engine
Intake Camshaft Position System Performance Bank 1 | DTC P0011, P0014, P0021, or P0024 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0013 | Exhaust Camshaft Position Actuator Solenoid Control Circuit | ECM | DTC P0010 or P0013 for the 1.6L (LDE) and 1.8L (2H0) engine or DTC P0010, P0013, or P2088-P2091 for the 2.0L engine
Exhaust Camshaft Position Actuator Solenoid Control Circuit Bank 1 | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0014 | Exhaust Camshaft Position System Performance | ECM | DTC P0011 or P0014 for the 1.6L (LDE) and 1.8L (2H0) engine
Exhaust Camshaft Position System Performance Bank 1 | DTC P0011, P0014, P0021, or P0024 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0016 | Crankshaft Position - Camshaft Position Correlation | ECM | DTC P0016, P0340, or P0341 for the 2.0L (Diesel) engine
Crankshaft Position - Intake Camshaft Position Correlation | DTC P0016 or P0017 for the 1.6L (LDE) and 1.8L (2H0) engine or DTC P0016 or P0017 for the 2.0L engine
Crankshaft Position - Intake Camshaft Position Correlation Bank 1 | DTC P0016, P0017, P0018, or P0019 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0017 | Crankshaft Position - Exhaust Camshaft Position Correlation | ECM | DTC P0016 or P0017 for the 1.6L (LDE) and 1.8L (2H0) engine or DTC P0016 or P0017 for the 2.0L engine
Crankshaft Position - Exhaust Camshaft Position Correlation Bank 1 | DTC P0011, P0014, P0021, or P0024 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0018 | Crankshaft Position - Intake Camshaft Position Correlation Bank 2 | ECM | DTC P0011, P0014, P0021, or P0024
P0019 | Crankshaft Position - Exhaust Camshaft Position Correlation Bank 2 | ECM | DTC P0011, P0014, P0021, or P0024
P0020 | Intake Camshaft Position Actuator Solenoid Control Circuit Bank 2 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P0021 | Intake Camshaft Position System Performance Bank 2 | ECM | DTC P0011, P0014, P0021, or P0024
P0023 | Exhaust Camshaft Position Actuator Solenoid Control Circuit Bank 2 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P0024 | Exhaust Camshaft Position System Performance Bank 2 | ECM | DTC P0011, P0014, P0021, or P0024
P0030 | HO2S Heater Control Circuit Sensor 1 | ECM |

• | DTC P0030, P0036, P0053, P0054, P0135, or P0141 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0030, P0031, P0032, P0053, or P0135 for the 2.0L engine

• | DTC P0030-P0032 for the 2.0L (Diesel) engine

• | DTC P0030, P0031, P0032, P0036, P0037, or P0038 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P0031 | HO2S Heater Control Circuit Low Voltage Sensor 1 | ECM |

• | DTC P0030, P0031, P0032, P0053, or P0135 for the 2.0L engine

• | DTC P0030-P0032 for the 2.0L (Diesel) engine

• | DTC P0030, P0031, P0032, P0036, P0037, or P0038 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P0032 | HO2S Heater Control Circuit High Voltage Sensor 1 | ECM |

• | DTC P0030, P0031, P0032, P0053, or P0135 for the 2.0L engine

• | DTC P0030-P0032 for the 2.0L (Diesel) engine

• | DTC P0030, P0031, P0032, P0036, P0037, or P0038 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P0033 | Turbocharger Bypass Valve Solenoid Control Circuit | ECM | DTC P0033, P0034, or P0035 for the 2.0L engine or DTC P0033, P0034, or P0035 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0034 | Turbocharger Bypass Valve Solenoid Control Circuit Low Voltage | ECM | DTC P0033, P0034, or P0035 for the 2.0L engine or DTC P0033, P0034, or P0035 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0035 | Turbocharger Bypass Valve Solenoid Control Circuit High Voltage | ECM | DTC P0033, P0034, or P0035 for the 2.0L engine or DTC P0033, P0034, or P0035 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0036 | HO2S Heater Control Circuit Sensor 2 | ECM |

• | DTC P0030, P0036, P0053, P0054, P0135, or P0141 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0036, P0037, P0038, or P0141 for the 2.0L engine

• | DTC P0030, P0031, P0032, P0036, P0037, or P0038 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P0037 | HO2S Heater Control Circuit Low Voltage Sensor 2 | ECM | DTC P0036, P0037, P0038, or P0141 for the 2.0L engine or DTC P0030, P0031, P0032, P0036, P0037, or P0038 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0038 | HO2S Heater Control Circuit High Voltage Sensor 2 | ECM | DTC P0036, P0037, P0038, or P0141 for the 2.0L engine or DTC P0030, P0031, P0032, P0036, P0037, or P0038 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P003A | Turbocharger Boost Control Position Not Learned | ECM | DTC P003A
P0045 | Turbocharger Boost Control Solenoid Control Circuit | ECM | DTC P0045-P0048
P0046 | Turbocharger Boost Pressure Output Circuit High Temperature | ECM | DTC P0045-P0048
P0047 | Turbocharger Boost Control Solenoid Control Circuit Low Voltage | ECM | DTC P0045-P0048
P0048 | Turbocharger Boost Control Solenoid Control Circuit High Voltage | ECM | DTC P0045-P0048
P0053 | HO2S Heater Resistance Sensor 1 | ECM | DTC P0030, P0036, P0053, P0054, P0135, or P0141 for the 1.6L (LDE) and 1.8L (2H0) engine or DTC P0030, P0031, P0032, P0053, or P0135 for the 2.0L engine
P0054 |  | ECM | DTC P0030, P0036, P0053, P0054, P0135, or P0141
P0068 | Throttle Body Airflow Performance | ECM | DTC P0068 or P1101
P0069 | Manifold Absolute Pressure - Barometric Pressure Correlation | ECM | DTC P0069
P0087 | Fuel Rail Pressure Too Low | ECM | DTC P0087, P0088, or P0089 for the 2.0L engine or DTC P0087 or P0088 for the 2.0L (Diesel) engine
P0088 | Fuel Rail Pressure Too High | ECM | DTC P0087, P0088, or P0089 for the 2.0L engine or DTC P0087 or P0088 for the 2.0L (Diesel) engine
P0089 | Fuel Pressure Regulator Performance | ECM | DTC P0087, P0088, or P0089
P0090 | Fuel Pressure Regulator Solenoid 1 Control Circuit | ECM | DTC P0090, P0091, or P0092
P0091 | Fuel Pressure Regulator Solenoid 1 Control Circuit Low Voltage | ECM | DTC P0090, P0091, or P0092
P0092 | Fuel Pressure Regulator Solenoid 1 Control Circuit High Voltage | ECM | DTC P0090, P0091, or P0092
P0097 | Intake Air Temperature Sensor 2 Low Voltage | ECM | DTC P0097, P0098, or P0099 for the 2.0L engine or DTC P0097 or P0098 for the 2.0L (Diesel) engine
P0098 | Intake Air Temperature Sensor 2 High Voltage | ECM | DTC P0097, P0098, or P0099 for the 2.0L engine or DTC P0097 or P0098 for the 2.0L (Diesel) engine
P0099 | Intake Air Temperature Sensor 2 Intermittent | ECM | DTC P0097, P0098, or P0099
P00B3 | Radiator Coolant Temperature Sensor Circuit Low Voltage | ECM | DTC P00B3 or P00B4
P00B4 | Radiator Coolant Temperature Sensor Circuit High Voltage | ECM | DTC P00B3 or P00B4
P00B6 | Radiator Coolant Temperature - Engine Coolant Temperature Not Plausible | ECM | DTC P00B6
P00B7 | Engine Coolant Flow Insufficient | ECM | DTC P00B7
P0100 | Mass Air Flow Sensor Circuit | ECM | DTC P0100, P0102, or P0103 for the 2.0L engine or DTC P0100, P0102, or P0103 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0101 | Mass Air Flow Sensor Performance | ECM |

• | DTC P0101 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0101 for the 2.0L engine

• | DTC P0101 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

Mass Air Flow Sensor Slip Detected | DTC P0101, P0102, or P0103 for the 2.0L (Deisel) engine
P0102 | Mass Air Flow Sensor Circuit Low Frequency | ECM |

• | DTC P0102 or P0103 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0100, P0102, or P0103 for the 2.0L engine

• | DTC P0100, P0102, or P0103 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

Mass Air Flow Sensor Circuit Low Low Input | DTC P0101, P0102, or P0103 for the 2.0L (Deisel) engine
P0103 | Mass Air Flow Sensor Circuit High Frequency | ECM |

• | DTC P0102 or P0103 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0100, P0102, or P0103 for the 2.0L engine

• | DTC P0100, P0102, or P0103 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

Mass Air Flow Sensor Circuit High High Input | DTC P0101, P0102, or P0103 for the 2.0L (Deisel) engine
P0106 | Manifold Absolute Pressure Sensor Performance | ECM | DTC P0106 for the 1.6L (LDE) and 1.8L (2H0) engine or DTC P0106 for the 2.0L engine
P0107 | Manifold Absolute Pressure Sensor Circuit Low Voltage | ECM |

• | DTC P0107 or P0108 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0107 or P0108 for the 2.0L engine

• | DTC P0107 or P0108 for the 2.0L (Deisel) engine

P0108 | Manifold Absolute Pressure Sensor Circuit High Voltage | ECM |

• | DTC P0107 or P0108 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0107 or P0108 for the 2.0L engine

• | DTC P0107 or P0108 for the 2.0L (Deisel) engine

P0112 | Intake Air Temperature Sensor Circuit Low Voltage | ECM |

• | DTC P0112 or P0113 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0112, P0113, or P0114 for the 2.0L engine

• | DTC P0112 or P0113 for the 2.0L (Deisel) engine

• | DTC P0112, P0113, or P0114 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P0113 | Intake Air Temperature Sensor Circuit High Voltage | ECM |

• | DTC P0112 or P0113 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0112, P0113, or P0114 for the 2.0L engine

• | DTC P0112 or P0113 for the 2.0L (Deisel) engine

• | DTC P0112, P0113, or P0114 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P0114 | Intake Air Temperature Sensor Circuit Intermittent | ECM | DTC P0112, P0113, or P0114 for the 2.0L engine or DTC P0112, P0113, or P0114 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0116 | Engine Coolant Temperature Sensor Performance | ECM | DTC P0116 for the 2.0L engine or DTC P0116 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0117 | Engine Coolant Temperature Sensor Circuit Low Voltage | ECM |

• | DTC P0117 or P0118 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0117, P0118, or P0119 for the 2.0L engine

• | DTC P0117 or P0118 for the 2.0L (Deisel) engine

• | DTC P0117 or P0118 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P0118 | Engine Coolant Temperature Sensor Circuit High Voltage | ECM |

• | DTC P0117 or P0118 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0117, P0118, or P0119 for the 2.0L engine

• | DTC P0117 or P0118 for the 2.0L (Deisel) engine

• | DTC P0117 or P0118 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P0119 | Engine Coolant Temperature Sensor Circuit Intermittent | ECM | DTC P0117, P0118, or P0119 for the 2.0L engine or DTC P0119 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0120 | Throttle Position Sensor 1 Circuit | ECM | DTC P0120-P0123, P0220, P0222, P0223, or P2135
P0121 | Throttle Position Sensor 1 Performance | ECM |

• | DTC P0120-P0123, P0220, P0222, P0223, or P2135 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0121, P0122, or P0123 for the 2.0L engine

• | DTC P0121, P0122, P0123, P0221, P0222, or P0223 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P0122 | Throttle Position Sensor 1 Circuit Low Voltage | ECM |

• | DTC P0120-P0123, P0220, P0222, P0223, or P2135 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0121, P0122, or P0123 for the 2.0L engine

• | DTC P0122 or P0123 for the 2.0L (Deisel) engine

• | DTC P0121, P0122, P0123, P0221, P0222, or P0223 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P0123 | Throttle Position Sensor 1 Circuit High Voltage | ECM |

• | DTC P0120-P0123, P0220, P0222, P0223, or P2135 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0121, P0122, or P0123 for the 2.0L engine

• | DTC P0122 or P0123 for the 2.0L (Deisel) engine

• | DTC P0121, P0122, P0123, P0221, P0222, or P0223 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P0130 | HO2S Circuit Closed Loop Performance Sensor 1 | ECM | DTC P0130, P0131, P0132, P0133, P2195, P2196, P2231, or P2297 for the 2.0L engine
HO2S Signal Circuit Shorted to Heater Circuit Sensor 1 | DTC P0130 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0131 | HO2S Circuit Low Voltage Sensor 1 | ECM |

• | DTC P0131, P0132, P0137, or P0138 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0130, P0131, P0132, P0133, P2195, P2196, P2231, or P2297 for the 2.0L engine

• | DTC P0131, P0132, or P0134 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

HO2S Circuit Sensor 1 Low Input | DTC P0131 or P0132 for the 2.0L (Deisel) engine
P0132 | HO2S Circuit High Voltage Sensor 1 | ECM |

• | DTC P0131, P0132, P0137, or P0138 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0130, P0131, P0132, P0133, P2195, P2196, P2231, or P2297 for the 2.0L engine

• | DTC P0131, P0132, or P0134 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

HO2S Circuit Sensor 1 High Input | DTC P0131 or P0132 for the 2.0L (Deisel) engine
P0133 | HO2S Slow Response Sensor 1 | ECM |

• | DTC P0133, P0134, P013A, P013B, P013E, P013F, P0140, P1133, P2270, P2271, or P2A00 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0130, P0131, P0132, P0133, P2195, P2196, P2231, or P2297 for the 2.0L engine

• | DTC P0133 for the 2.0L (Deisel) engine

• | DTC P0133 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P0134 | HO2S Circuit Insufficient Activity Sensor 1 | ECM | DTC P0133, P0134, P013A, P013B, P013E, P013F, P0140, P1133, P2270, P2271, or P2A00 for the 1.6L (LDE) and 1.8L (2H0) engine or DTC P0131, P0132, or P0134 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0135 | HO2S Heater Performance Sensor 1 | ECM |

• | DTC P0030, P0036, P0053, P0054, P0135, or P0141 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0030, P0031, P0032, P0053, or P0135 for the 2.0L engine

• | DTC P0135 or P0141 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P0137 | HO2S Circuit Low Voltage Sensor 2 | ECM |

• | DTC P0131, P0132, P0137, or P0138 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0137, P0138, P0140, P2232, P2270, or P2271 for the 2.0L engine

• | DTC P0137, P0138, or P0140 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P0138 | HO2S Circuit High Voltage Sensor 2 | ECM |

• | DTC P0131, P0132, P0137, or P0138 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0137, P0138, P0140, P2232, P2270, or P2271 for the 2.0L engine

• | DTC P0137, P0138, or P0140 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P013A | HO2S Slow Response Rich to Lean Sensor 2 | ECM | DTC P0133, P0134, P013A, P013B, P013E, P013F, P0140, P1133, P2270, P2271, or P2A00
P013B | HO2S Slow Response Lean to Rich Sensor 2 | ECM | DTC P0133, P0134, P013A, P013B, P013E, P013F, P0140, P1133, P2270, P2271, or P2A00
P013E | HO2S Delayed Response Rich to Lean Sensor 2 | ECM | DTC P0133, P0134, P013A, P013B, P013E, P013F, P0140, P1133, P2270, P2271, or P2A00
P013F | HO2S Delayed Response Lean to Rich Sensor 2 | ECM | DTC P0133, P0134, P013A, P013B, P013E, P013F, P0140, P1133, P2270, P2271, or P2A00
P0140 | HO2S Circuit Insufficient Activity Sensor 2 | ECM |

• | DTC P0133, P0134, P013A, P013B, P013E, P013F, P0140, P1133, P2270, P2271, or P2A00 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0137, P0138, P0140, P2232, P2270, or P2271 for the 2.0L engine

• | DTC P0137, P0138, or P0140 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P0141 | HO2S Heater Performance Sensor 2 | ECM |

• | DTC P0030, P0036, P0053, P0054, P0135, or P0141 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0036, P0037, P0038, or P0141 for the 2.0L engine

• | DTC P0135 or P0141 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P0171 | Fuel Trim System Lean | ECM | DTC P0171 or P0172
P0172 | Fuel Trim System Rich | ECM | DTC P0171 or P0172
P0182 | Fuel Temperature Sensor Circuit Low Voltage | ECM | DTC P0182 or P0183 for the 2.0L (Deisel) engine
P0183 | Fuel Temperature Sensor Circuit High Voltage | ECM | DTC P0182 or P0183 for the 2.0L (Deisel) engine
P0191 | Fuel Rail Pressure Sensor Performance | ECM | DTC P0191 for the 2.0L engine or DTC P0191 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0192 | Fuel Rail Pressure Sensor Circuit Low Voltage | ECM |

• | DTC P0192 or P0193 for the 2.0L engine

• | DTC P0192 or P0193 for the 2.0L (Deisel) engine

• | DTC P0192 or P0193 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P0193 | Fuel Rail Pressure Sensor Circuit High Voltage | ECM |

• | DTC P0192 or P0193 for the 2.0L engine

• | DTC P0192 or P0193 for the 2.0L (Deisel) engine

• | DTC P0192 or P0193 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P0194 | Fuel Rail Pressure Sensor Circuit Erratic | ECM | DTC P0194 for the 2.0L (Deisel) engine
P0201 | Cylinder 1 Injector Control Circuit | ECM | DTC P0201, P0202, P0203, or P0204 for the 1.6L (LDE) and 1.8L (2H0) engine
Injector 1 Control Circuit | DTC P0201-P0204, P0261, P0264, P0267, P0270, or P2146-P2157 for the 2.0L engine or DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Fuel Injector 1 Control Circuit | DTC P0201, P0202, P0203, or P0204 for the 2.0L (Deisel) engine
P0202 | Cylinder 2 Injector Control Circuit | ECM | DTC P0201, P0202, P0203, or P0204 for the 1.6L (LDE) and 1.8L (2H0) engine
Injector 2 Control Circuit | DTC P0201-P0204, P0261, P0264, P0267, P0270, or P2146-P2157 for the 2.0L engine or DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Fuel Injector 2 Control Circuit | DTC P0201, P0202, P0203, or P0204 for the 2.0L (Deisel) engine
P0203 | Cylinder 3 Injector Control Circuit | ECM | DTC P0201, P0202, P0203, or P0204 for the 1.6L (LDE) and 1.8L (2H0) engine
Injector 3 Control Circuit | DTC P0201-P0204, P0261, P0264, P0267, P0270, or P2146-P2157 for the 2.0L engine or DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Fuel Injector 3 Control Circuit | DTC P0201, P0202, P0203, or P0204 for the 2.0L (Deisel) engine
P0204 | Cylinder 4 Injector Control Circuit | ECM | DTC P0201, P0202, P0203, or P0204 for the 1.6L (LDE) and 1.8L (2H0) engine
Injector 4 Control Circuit | DTC P0201-P0204, P0261, P0264, P0267, P0270, or P2146-P2157 for the 2.0L engine or DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Fuel Injector 4 Control Circuit | DTC P0201, P0202, P0203, or P0204 for the 2.0L (Deisel) engine
P0205 | Injector 5 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0206 | Injector 6 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0218 | Transmission Fluid Overtemperature | TCM | DTC P0218
P0219 | Engine Overspeed | ECM | DTC P0219 for the 2.0L (Deisel) engine or DTC P0219 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0220 | Throttle Position Sensor 2 Circuit | ECM | DTC P0120-P0123, P0220, P0222, P0223, or P2135
P0221 | Throttle Position Sensor 2 Performance | ECM | DTC P0221, P0222, or P0223 for the 2.0L engine or DTC P0121, P0122, P0123, P0221, P0222, or P0223 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0222 | Throttle Position Sensor 2 Circuit Low Voltage | ECM |

• | DTC P0120-P0123, P0220, P0222, P0223, or P2135 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0221, P0222, or P0223 for the 2.0L engine

• | DTC P0121, P0122, P0123, P0221, P0222, or P0223 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P0223 | Throttle Position Sensor 2 Circuit High Voltage | ECM |

• | DTC P0120-P0123, P0220, P0222, P0223, or P2135 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0221, P0222, or P0223 for the 2.0L engine

• | DTC P0121, P0122, P0123, P0221, P0222, or P0223 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P0230 | Fuel Pump Relay Control Circuit | ECM | DTC P0230
P0231 | Fuel Pump Control Circuit Low Voltage | ECM | DTC P0231, P0232, or P023F for the 2.0L engine or DTC P0231, P0232, or P023F for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0232 | Fuel Pump Control Circuit High Voltage | ECM | DTC P0231, P0232, or P023F for the 2.0L engine or DTC P0231, P0232, or P023F for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0234 | Turbocharger Engine Overboost | ECM |

• | DTC P0234 or P0299 for the 2.0L engine

• | DTC P0234 or P0299 for the 2.0L (Deisel) engine

• | DTC P0234 or P0299 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P023F | Fuel Pump Control Circuit | ECM | DTC P0231, P0232, or P023F for the 2.0L engine or DTC P0231, P0232, or P023F for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0236 | Turbocharger Boost System Performance | ECM | DTC P0236, P0237, or P0238 for the 2.0L engine or DTC P0236, P0237, or P0238 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0237 | Turbocharger Boost Sensor Circuit Low Voltage | ECM | DTC P0236, P0237, or P0238 for the 2.0L engine or DTC P0236, P0237, or P0238 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0238 | Turbocharger Boost Sensor Circuit High Voltage | ECM | DTC P0236, P0237, or P0238 for the 2.0L engine or DTC P0236, P0237, or P0238 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0244 | Turbocharger Wastegate Solenoid Control Performance | ECM | DTC P0244-P0246 for the 2.0L engine or DTC P0244-P0246 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0245 | Turbocharger Wastegate Solenoid Control Circuit Low Voltage | ECM | DTC P0244-P0246 for the 2.0L engine or DTC P0244-P0246 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0246 | Turbocharger Wastegate Solenoid Control Circuit High Voltage | ECM | DTC P0244-P0246 for the 2.0L engine or DTC P0244-P0246 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0251 | Fuel Pressure Regulator Control Circuit Malfunction | ECM | DTC P0251-P0254, P0258, or P0259 for the 2.0L (Deisel) engine
P0252 | Fuel Pressure Regulator Performance | ECM | DTC P0251-P0254, P0258, or P0259 for the 2.0L (Deisel) engine
P0253 | Fuel Pressure Regulator Control Circuit Low Voltage | ECM | DTC P0251-P0254, P0258, or P0259 for the 2.0L (Deisel) engine
P0254 | Fuel Pressure Regulator Control Circuit High Voltage | ECM | DTC P0251-P0254, P0258, or P0259 for the 2.0L (Deisel) engine
P025A | Fuel Pump Flow Control Module Enable Circuit | ECM | DTC P025A for the 2.0L engine or DTC P025A for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0261 | Cylinder 1 Injector Control Circuit Low Voltage | ECM | DTC P0201-P0204, P0261, P0264, P0267, P0270, or P2146-P2157 for the 2.0L engine or DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Injector 1 Control Circuit Low Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.0L (Deisel) engine
P0262 | Cylinder 1 Injector Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Injector 1 Control Circuit High Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.0L (Deisel) engine
P0264 | Cylinder 2 Injector Control Circuit Low Voltage | ECM | DTC P0201-P0204, P0261, P0264, P0267, P0270, or P2146-P2157 for the 2.0L engine or DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Injector 2 Control Circuit Low Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.0L (Deisel) engine
P0265 | Cylinder 2 Injector Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Injector 2 Control Circuit High Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.0L (Deisel) engine
P0267 | Cylinder 3 Injector Control Circuit Low Voltage | ECM | DTC P0201-P0204, P0261, P0264, P0267, P0270, or P2146-P2157 for the 2.0L engine or DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Injector 3 Control Circuit Low Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.0L (Deisel) engine
P0268 | Cylinder 3 Injector Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Injector 3 Control Circuit High Voltage | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.0L (Deisel) engine
P0270 | Cylinder 4 Injector Control Circuit Low Voltage | ECM | DTC P0201-P0204, P0261, P0264, P0267, P0270, or P2146-P2157 for the 2.0L engine or DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Injector 4 Control Circuit Low Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.0L (Deisel) engine
P0271 | Cylinder 4 Injector Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Injector 4 Control Circuit High Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.0L (Deisel) engine
P0273 | Cylinder 5 Injector Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0274 | Cylinder 5 Injector Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0276 | Cylinder 6 Injector Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0277 | Cylinder 6 Injector Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0299 | Turbocharger Engine Underboost | ECM |

• | DTC P0234 or P0299 for the 2.0L engine

• | DTC P0234 or P0299 for the 2.0L (Deisel) engine

• | DTC P0234 or P0299 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P0300 | Engine Misfire Detected | ECM |

• | DTC P0300-P0304 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0300-P0304 for the 2.0L engine

• | DTC P0300-P0306 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P0301 | Cylinder 1 Misfire Detected | ECM |

• | DTC P0300-P0304 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0300-P0304 for the 2.0L engine

• | DTC P0300-P0306 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P0302 | Cylinder 2 Misfire Detected | ECM |

• | DTC P0300-P0304 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0300-P0304 for the 2.0L engine

• | DTC P0300-P0306 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P0303 | Cylinder 3 Misfire Detected | ECM |

• | DTC P0300-P0304 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0300-P0304 for the 2.0L engine

• | DTC P0300-P0306 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P0304 | Cylinder 4 Misfire Detected | ECM |

• | DTC P0300-P0304 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0300-P0304 for the 2.0L engine

• | DTC P0300-P0306 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P0305 | Cylinder 5 Misfire Detected | ECM | DTC P0300-P0306
P0306 | Cylinder 6 Misfire Detected | ECM | DTC P0300-P0306
P0313 | Misfire Detected With Low Fuel Level | ECM | DTC P0313
P0315 | Crankshaft Position System Variation Not Learned | ECM | DTC P0315
P0324 | Knock Sensor Performance | ECM | DTC P0324, P0326, P0327, P0328, P0331, P0332, or P0333 for the 2.0L engine
Knock Sensor Module Performance | DTC P0324
P0325 | Knock Sensor Circuit | ECM | DTC P0325, P0327, or P0328
P0326 | Knock Sensor Performance | ECM | DTC P0326 or P06B6 for the 1.6L (LDE) and 1.8L (2H0) engine
Knock Sensor 1 Performance | DTC P0324, P0326, P0327, P0328, P0331, P0332, or P0333 for the 2.0L engine
Knock Sensor System Performance Bank 1 | DTC P0326, P0327, P0328, P0331, P0332, or P0333 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0327 | Knock Sensor Circuit Low Voltage | ECM | DTC P0325, P0327, or P0328 for the 1.6L (LDE) and 1.8L (2H0) engine
Knock Sensor 1 Circuit Low Voltage | DTC P0324, P0326, P0327, P0328, P0331, P0332, or P0333 for the 2.0L engine
Knock Sensor Circuit Low Voltage Bank 1 | DTC P0326, P0327, P0328, P0331, P0332, or P0333 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0328 | Knock Sensor Circuit High Voltage | ECM | DTC P0325, P0327, or P0328 for the 1.6L (LDE) and 1.8L (2H0) engine
Knock Sensor 1 Circuit High Voltage | DTC P0324, P0326, P0327, P0328, P0331, P0332, or P0333 for the 2.0L engine
Knock Sensor Circuit High Voltage Bank 1 | DTC P0326, P0327, P0328, P0331, P0332, or P0333 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0331 | Knock Sensor 2 Performance | ECM | DTC P0324, P0326, P0327, P0328, P0331, P0332, or P0333 for the 2.0L engine
Knock Sensor System Performance Bank 2 | DTC P0326, P0327, P0328, P0331, P0332, or P0333 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0332 | Knock Sensor 2 Circuit Low Voltage | ECM | DTC P0324, P0326, P0327, P0328, P0331, P0332, or P0333 for the 2.0L engine
Knock Sensor Circuit Low Voltage Bank 2 | DTC P0326, P0327, P0328, P0331, P0332, or P0333 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0333 | Knock Sensor 2 Circuit High Voltage | ECM | DTC P0324, P0326, P0327, P0328, P0331, P0332, or P0333 for the 2.0L engine
Knock Sensor Circuit High Voltage Bank 2 | DTC P0326, P0327, P0328, P0331, P0332, or P0333 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0335 | Crankshaft Position Sensor Circuit | ECM |

• | DTC P0335 or P0336 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0335, P0336, or P0338 for the 2.0L engine

• | DTC P0335, P0336, or P0338 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P0336 | Crankshaft Position Sensor Performance | ECM |

• | DTC P0335 or P0336 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0335, P0336, or P0338 for the 2.0L engine

• | DTC P0336 for the 2.0L (Diesel) engine

• | DTC P0335, P0336, or P0338 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P0338 | Crankshaft Position Sensor Circuit High Duty Cycle | ECM | DTC P0335, P0336, or P0338 for the 2.0L engine or DTC P0335, P0336, or P0338 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0340 | Intake Camshaft Position Sensor Circuit | ECM | DTC P0340 or P0365 for the 1.6L (LDE) and 1.8L (2H0) engine
Camshaft Position Sensor Circuit | DTC P0016, P0340, or P0341 for the 2.0L (Diesel) engine
P0341 | Intake Camshaft Position Sensor Performance | ECM | DTC P0341 or P0366 for the 1.6L (LDE) and 1.8L (2H0) engine or DTC P0341, P0342, or P0343 for the 2.0L engine
Intake Camshaft Position Sensor Performance Bank 1 | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Camshaft Position Sensor Performance | DTC P0016, P0340, or P0341 for the 2.0L (Diesel) engine
P0342 | Intake Camshaft Position Sensor Circuit Low Voltage | ECM | DTC P0341, P0342, or P0343 for the 2.0L engine
Intake Camshaft Position Sensor Circuit Low Voltage Bank 1 | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0343 | Intake Camshaft Position Sensor Circuit High Voltage | ECM | DTC P0341, P0342, or P0343 for the 2.0L engine
Intake Camshaft Position Sensor Circuit High Voltage Bank 1 | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0346 | Intake Camshaft Position Sensor Performance Bank 2 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0347 | Intake Camshaft Position Sensor Circuit Low Voltage Bank 2 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0348 | Intake Camshaft Position Sensor Circuit High Voltage Bank 2 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0351 | Ignition Coil 1 Control Circuit | ECM |

• | DTC P0351-P0354 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0351-P0354 for the 2.0L engine

• | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P0352 | Ignition Coil 2 Control Circuit | ECM |

• | DTC P0351-P0354 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0351-P0354 for the 2.0L engine

• | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P0353 | Ignition Coil 3 Control Circuit | ECM |

• | DTC P0351-P0354 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0351-P0354 for the 2.0L engine

• | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P0354 | Ignition Coil 4 Control Circuit | ECM |

• | DTC P0351-P0354 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0351-P0354 for the 2.0L engine

• | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P0355 | Ignition Coil 5 Control Circuit | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P0356 | Ignition Coil 6 Control Circuit | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P0365 | Exhaust Camshaft Position Sensor Circuit | ECM | DTC P0340 or P0365
P0366 | Exhaust Camshaft Position Sensor Performance | ECM | DTC P0341 or P0366 for the 1.6L (LDE) and 1.8L (2H0) engine or DTC P0366, P0367, or P0368 for the 2.0L engine
Exhaust Camshaft Position Sensor Performance Bank 1 | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0367 | Exhaust Camshaft Position Sensor Circuit Low Voltage | ECM | DTC P0366, P0367, or P0368 for the 2.0L engine
Exhaust Camshaft Position Sensor Circuit Low Voltage Bank 1 | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0368 | Exhaust Camshaft Position Sensor Circuit High Voltage | ECM | DTC P0366, P0367, or P0368 for the 2.0L engine
Exhaust Camshaft Position Sensor Circuit High Voltage Bank 1 | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0380 | Glow Plug Feedback Circuit Malfunction | ECM | DTC P0380, P0383, or P0134
P0383 | Glow Plug Feedback Circuit Low Voltage | ECM | DTC P0380, P0383, or P0134
P0384 | Glow Plug Feedback Circuit High Voltage | ECM | DTC P0380, P0383, or P0134
P0391 | Exhaust Camshaft Position Sensor Performance Bank 2 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0392 | Exhaust Camshaft Position Sensor Circuit Low Voltage Bank 2 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0393 | Exhaust Camshaft Position Sensor Circuit High Voltage Bank 2 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0401 | Exhaust Gas Recirculation Flow Insufficient | ECM | DTC P0401 or P0402
P0402 | Exhaust Gas Recirculation Flow Excessive | ECM | DTC P0401 or P0402
P0403 | Exhaust Gas Recirculation Control Circuit | ECM | DTC P0403, P0489, or P0490
P0404 | Exhaust Gas Recirculation Control Circuit | ECM | DTC P0404
P0405 | Exhaust Gas Recirculation Position Sensor Circuit Low Voltage | ECM | DTC P0405 or P0406
P0406 | Exhaust Gas Recirculation Position Sensor Circuit High Voltage | ECM | DTC P0405 or P0406
P0411 | Secondary Air Injection System Incorrect Air Flow Detected | ECM | DTC P0411
P0418 | Secondary Air Injection Pump Control Circuit | ECM | DTC P0418, P2444, or P2445
P0420 | Catalyst System Low Efficiency | ECM |

• | DTC P0420 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0420 for the 2.0L engine

• | DTC P0420 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P0443 | Evaporative Emission Purge Solenoid Valve Control Circuit | ECM |

• | DTC P0443 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0443, P0458, or P0459 for the 2.0L engine

• | DTC P0443, P0458, or P0459 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P0458 | Evaporative Emission Purge Solenoid Control Circuit Low Voltage | ECM | DTC P0443, P0458, or P0459 for the 2.0L engine or DTC P0443, P0458, or P0459 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0459 | Evaporative Emission Purge Solenoid Control Circuit High Voltage | ECM | DTC P0443, P0458, or P0459 for the 2.0L engine or DTC P0443, P0458, or P0459 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0461 | Fuel Level Sensor Circuit Performance | ECM | DTC P0461-P0463, P2066, P2067, or P2068
P0462 | Fuel Level Sensor Circuit Low Voltage | ECM | DTC P0461-P0463, P2066, P2067, or P2068
P0463 | Fuel Level Sensor Circuit High Voltage | ECM | DTC P0461-P0463, P2066, P2067, or P2068
P0480 | Cooling Fan Relay 1 Control Circuit | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694 for 4 cyl or V6 engines or DTC P0480-P0482 or P0691-P0696
P0481 | Cooling Fan Relay 2 Control Circuit | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694 for 4 cyl or V6 engines or DTC P0480-P0482 or P0691-P0696
P0482 | Cooling Fan Relay 3 Control Circuit | ECM | DTC P0480-P0482 or P0691-P0696
P0489 | Exhaust Gas Recirculation Motor Control Circuit Low Input | ECM | DTC P0403, P0489, or P0490
P0490 | Exhaust Gas Recirculation Motor Control Circuit High Input | ECM | DTC P0403, P0489, or P0490
P0500 | Vehicle Speed Sensor Circuit | TCM | DTC P0500-P0503
P0501 | Vehicle Speed Sensor Performance | TCM | DTC P0500-P0503
P0502 | Vehicle Speed Sensor Circuit Low Voltage | TCM | DTC P0500-P0503
P0503 | Vehicle Speed Sensor Circuit Intermittent | TCM | DTC P0500-P0503
P0506 | Idle Speed Low | ECM | DTC P0506 or P0507
P0507 | Idle Speed High | ECM | DTC P0506 or P0507
P050A | Cold Start Idle Air Control System Performance | ECM | DTC P050A
P0513 | Immobilizer Key Incorrect | ECM | DTC P0513
P0520 | Engine Oil Pressure Switch Circuit Malfunction | ECM | DTC P0520
P0521 | Engine Oil Pressure Sensor Performance | ECM | DTC P0521, P0522, or P0523
P0522 | Engine Oil Pressure Sensor Circuit Low Voltage | ECM | DTC P0521, P0522, or P0523
P0523 | Engine Oil Pressure Sensor Circuit High Voltage | ECM | DTC P0521, P0522, or P0523
P052E | Positive Crankcase Ventilation Heater Control Circuit Performance | ECM | DTC P052E or P053A-P053C
P0531 | Air Conditioning Pressure Sensor Sensor Performance | ECM | DTC P0531, P0532, or P0533 with CJ2 or C68 or DTC P0531, P0532, or P0533 with C67
P0532 | Air Conditioning Pressure Sensor Circuit Low Voltage | ECM | DTC P0531, P0532, or P0533 with CJ2 or C68 or DTC P0531, P0532, or P0533 with C67
P0533 | Air Conditioning Pressure Sensor Circuit High Voltage | ECM | DTC P0531, P0532, or P0533 with CJ2 or C68 or DTC P0531, P0532, or P0533 with C67
P053A | Positive Crankcase Ventilation Heater Control Circuit Open | ECM | DTC P052E or P053A-P053C
P053B | Positive Crankcase Ventilation Heater Control Circuit Low Voltage | ECM | DTC P052E or P053A-P053C
P053C | Positive Crankcase Ventilation Heater Control Circuit High Voltage | ECM | DTC P052E or P053A-P053C
P0560 | System Voltage | ECM | DTC P0560
P0562 | System Voltage Low | ECM | DTC P0562
P0563 | System Voltage High | ECM | DTC P0563
P0572 | Brake Switch Circuit 1 Low Voltage | ECM | DTC P0572 or P0573
P0573 | Brake Switch Circuit 1 High Voltage | ECM | DTC P0572 or P0573
P0575 | Cruise Control Switch Signal Circuit | ECM | DTC P0575
P0597 | Engine Coolant Thermostat Heater Control Circuit | ECM | DTC P0597-P0599
P0598 | Engine Coolant Thermostat Heater Control Circuit Low Voltage | ECM | DTC P0597-P0599
P0599 | Engine Coolant Thermostat Heater Control Circuit High Voltage | ECM | DTC P0597-P0599
P0601 | Control Module Read Only Memory | ECM | DTC P0601-P0604, P0606, P0607, P060D P062F, P16F3, or P2610 for the 1.6L (LDE) and 1.8L (2H0) engine or DTC P0601-P0606, P062B, P064D, P167A, P167D, P2105, or P2610 for the 2.0L engine
Fuel Pump Control Module | DTC P0601-P0604, P0606, or P062F for the 2.0L engine or DTC P0601-P0604, P0606, or P062F for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0602 | Control Module Not Programmed | ECM |

• | DTC P0601-P0604, P0606, P0607, P060D P062F, P16F3, or P2610 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0601-P0606, P062B, P064D, P167A, P167D, P2105, or P2610 for the 2.0L engine

• | DTC P0602, P0605-P0607, P060A, P060B, P0610, P061A, P061C, P062B, or P062F for the 2.0L (Diesel) engine

• | DTC P0602, P0610, P0614, P0630, P160D, P160E, or P161F for the 2.8L, 3.0L, 3.2L, or 3.6L engine

Fuel Pump Control Module | DTC P0601-P0604, P0606, or P062F for the 2.0L engine or DTC P0601-P0604, P0606, or P062F for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0603 | Control Module Long Term Memory Reset | ECM |

• | DTC P0601-P0604, P0606, P0607, P060D P062F, P16F3, or P2610 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0601-P0606, P062B, P064D, P167A, P167D, P2105, or P2610 for the 2.0L engine

• | DTC P0603-P0606 or P167D for the 2.8L, 3.0L, 3.2L, or 3.6L engine

Fuel Pump Control Module | DTC P0601-P0604, P0606, or P062F for the 2.0L engine or DTC P0601-P0604, P0606, or P062F for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0604 | Control Module Random Access Memory | ECM |

• | DTC P0601-P0604, P0606, P0607, P060D P062F, P16F3, or P2610 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0601-P0606, P062B, P064D, P167A, P167D, P2105, or P2610 for the 2.0L engine

• | DTC P0603-P0606 or P167D for the 2.8L, 3.0L, 3.2L, or 3.6L engine

Fuel Pump Control Module | DTC P0601-P0604, P0606, or P062F for the 2.0L engine or DTC P0601-P0604, P0606, or P062F for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0605 | Control Module Read Only Memory | ECM | DTC P0602, P0605-P0607, P060A, P060B, P0610, P061A, P061C, P062B, or P062F for the 2.0L (Diesel) engine or DTC P0603-P0606 or P167D for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0606 | Control Module Internal Performance | ECM |

• | DTC P0601-P0604, P0606, P0607, P060D P062F, P16F3, or P2610 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0601-P0606, P062B, P064D, P167A, P167D, P2105, or P2610 for the 2.0L engine

• | DTC P0603-P0606 or P167D for the 2.8L, 3.0L, 3.2L, or 3.6L engine

Fuel Pump Control Module | DTC P0601-P0604, P0606, or P062F for the 2.0L engine or DTC P0601-P0604, P0606, or P062F for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Control Module Processor Performance | ECM | DTC P0602, P0605-P0607, P060A, P060B, P0610, P061A, P061C, P062B, or P062F for the 2.0L (Diesel) engine
P0607 | Control Module Performance | ECM | DTC P0601-P0604, P0606, P0607, P060D P062F, P16F3, or P2610 for the 1.6L (LDE) and 1.8L (2H0) engine
Control Module Processor Performance | DTC P0602, P0605-P0607, P060A, P060B, P0610, P061A, P061C, P062B, or P062F for the 2.0L (Diesel) engine
P060A | Control Module Monitoring Processor Performance | ECM | DTC P0602, P0605-P0607, P060A, P060B, P0610, P061A, P061C, P062B, or P062F
P060B | Control Module Analog to Digital Converter Performance | ECM | DTC P0602, P0605-P0607, P060A, P060B, P0610, P061A, P061C, P062B, or P062F
P060D | Control Module Accelerator Pedal Position (APP) System Performance | ECM | DTC P0601-P0604, P0606, P0607, P060D P062F, P16F3, or P2610
P0610 | Control Module Programming Read Only Memory Performance Malfunction | ECM | DTC P0602, P0605-P0607, P060A, P060B, P0610, P061A, P061C, P062B, or P062F for the 2.0L (Diesel) engine
Control Module Vehicle Options Incorrect | DTC P0602, P0610, P0614, P0630, P160D, P160E, or P161F for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0614 | Engine Control Module/Transmission Control Module Programming Correlation | ECM | DTC P0602, P0610, P0614, P0630, P160D, P160E, or P161F
P0615 | Starter Relay Control Circuit | ECM | DTC P0615
P0616 | Starter Relay Control Circuit Low Voltage | ECM | DTC P0616
P0617 | Starter Relay Control Circuit High Voltage | ECM | DTC P0617
P061A | Control Module Torque Calculation Performance | ECM | DTC P0602, P0605-P0607, P060A, P060B, P0610, P061A, P061C, P062B, or P062F
P061C | Control Module Engine Speed System Circuitry Performance | ECM | DTC P0602, P0605-P0607, P060A, P060B, P0610, P061A, P061C, P062B, or P062F
P0621 | Generator L-Teminal Circuit | ECM | DTC P0621
P0625 | Generator F-Terminal Circuit Low Voltage | ECM | DTC P0625
P0626 | Generator F-Terminal Circuit High Voltage | ECM | DTC P0626
P0627 | Fuel Pump Relay Control Circuit | ECM | DTC P0627, P0628, or P0629 for the 2.0L engine or DTC P0627, P0628, or P0629 for the 2.0L (Diesel) engine
P0628 | Fuel Pump Relay Control Circuit Low Voltage | ECM | DTC P0627, P0628, or P0629 for the 2.0L engine or DTC P0627, P0628, or P0629 for the 2.0L (Diesel) engine
P0629 | Fuel Pump Relay Control Circuit High Voltage | ECM | DTC P0627, P0628, or P0629 for the 2.0L engine or DTC P0627, P0628, or P0629 for the 2.0L (Diesel) engine
P062A | Fuel Pump Relay Control Circuit Open | ECM | DTC P062A
P062B | Control Module Fuel Injector Control Performance | ECM | DTC P0601-P0606, P062B, P064D, P167A, P167D, P2105, or P2610 for the 2.0L engine or DTC P0602, P0605-P0607, P060A, P060B, P0610, P061A, P061C, P062B, or P062F for the 2.0L (Diesel) engine
P062D | Injector Positive Voltage Control Circuit Group 1 | ECM | DTC P062D or P062E
P062E | Injector Positive Voltage Control Circuit Group 2 | ECM | DTC P062D or P062E
P062F | Control Module Long Term Memory Performance | ECM | DTC P0601-P0604, P0606, P0607, P060D P062F, P16F3, or P2610 for the 1.6L (LDE) and 1.8L (2H0) engine
Fuel Pump Control Module | DTC P0601-P0604, P0606, or P062F for the 2.0L engine or DTC P0601-P0604, P0606, or P062F for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Control Module Long Term Memory Performance EEPROM Performance | ECM | DTC P0602, P0605-P0607, P060A, P060B, P0610, P061A, P061C, P062B, or P062F for the 2.0L (Diesel) engine
P0630 | VIN Not Programmed or Mismatched - Engine Control Module | ECM | DTC P0630 for the 2.0L (Diesel) engine or DTC P0602, P0610, P0614, P0630, P160D, P160E, or P161F for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0633 | Immobilizer Key Not Programmed | ECM | DTC P0633
P0638 | Throttle Actuator Control Command Performance | ECM | DTC P0641 for the 2.0L engine or DTC P0638, P2100-P2103, or P2119 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0641 | 5-Volt Reference 1 Circuit | ECM |

• | DTC P0641, P0651, P0697, or P06A3 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0641-P0643, P0651-P0653, or P0697-P0699 for the 2.0L engine

• | DTC P0630 for the 2.0L (Diesel) engine

• | DTC P0641-P0643, P0651-P0653, or P0697-P0699 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

5-Volt Reference Circuit | Fuel Pump Control Module | DTC P0641 or P06A6 for the 2.0L engine or DTC P0641 or P06A6 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0642 | 5-Volt Reference 1 Low Voltage | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699 for the 2.0L engine or DTC P0641-P0643, P0651-P0653, or P0697-P0699 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0643 | 5-Volt Reference 1 High Voltage | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699 for the 2.0L engine or DTC P0641-P0643, P0651-P0653, or P0697-P0699 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0645 | Air Conditioning Clutch Relay Control Circuit | ECM | DTC P0645, P0646, or P0647 with CJ2 or C68 or DTC P0645, P0646, or P0647 with C67
P0646 | Air Conditioning Clutch Relay Control Circuit Low Voltage | ECM | DTC P0645, P0646, or P0647 with CJ2 or C68 or DTC P0645, P0646, or P0647 with C67
P0647 | Air Conditioning Clutch Relay Control Circuit High Voltage | ECM | DTC P0645, P0646, or P0647 with CJ2 or C68 or DTC P0645, P0646, or P0647 with C67
P064A | Fuel Pump Flow Control Module Performance | Fuel Pump Control Module | DTC P1255 or P064A for the 2.0L engine or DTC P1255 or P064A for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P064C | Glow Plug Control Module Performance | ECM | DTC P064C
P064D | Control Module HO2S 1 System Performance | ECM | DTC P0601-P0606, P062B, P064D, P167A, P167D, P2105, or P2610 for the 2.0L engine or DTC P064D for the 2.0L (Diesel) engine
P0651 | 5-Volt Reference 2 Circuit | ECM |

• | DTC P0641, P0651, P0697, or P06A3 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0641-P0643, P0651-P0653, or P0697-P0699 for the 2.0L engine

• | DTC P0651 for the 2.0L (Diesel) engine

• | DTC P0641-P0643, P0651-P0653, or P0697-P0699 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P0652 | 5-Volt Reference 2 Low Voltage | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699 for the 2.0L engine or DTC P0641-P0643, P0651-P0653, or P0697-P0699 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0653 | 5-Volt Reference 2 High Voltage | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699 for the 2.0L engine or DTC P0641-P0643, P0651-P0653, or P0697-P0699 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0658 |  | ECM | DTC P0658 or P0659
P0659 |  | ECM | DTC P0658 or P0659
P0660 | Intake Manifold Tuning Valve Solenoid Control Circuit | ECM | DTC P0660
P066A | Cylinder 1 Glow Plug Control Circuit Low Voltage | ECM | DTC P0651
P066C | Cylinder 2 Glow Plug Control Circuit Low Voltage | ECM | DTC P0651
P066E | Cylinder 3 Glow Plug Control Circuit Low Voltage | ECM | DTC P0651
P06A6 | 5-Volt Reference Circuit Performance | Fuel Pump Control Module | DTC P0641 or P06A6 for the 2.0L engine or DTC P0641 or P06A6 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0671 | Cylinder 1 Glow Plug Control Circuit | ECM | DTC P0671, P0672, P0673, or P0674
P0672 | Cylinder 2 Glow Plug Control Circuit | ECM | DTC P0671, P0672, P0673, or P0674
P0673 | Cylinder 3 Glow Plug Control Circuit | ECM | DTC P0671, P0672, P0673, or P0674
P0674 | Cylinder 4 Glow Plug Control Circuit | ECM | DTC P0671, P0672, P0673, or P0674
P067A | Cylinder 4 Glow Plug Control Circuit Low Voltage | ECM | DTC P0651
P0685 | Engine Controls Ignition Relay Control Circuit | ECM |

• | DTC P0685, P0689, or P0690 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0685, P0686, P0687, P0689, or P0690 for the 2.0L engine

• | DTC P0685, P0686, P0687, P0689, or P0690 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P0686 | Engine Controls Ignition Relay Control Circuit Low Voltage | ECM | DTC P0685, P0686, P0687, P0689, or P0690 for the 2.0L engine or DTC P0685, P0686, P0687, P0689, or P0690 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0687 | Engine Controls Ignition Relay Control Circuit High Voltage | ECM | DTC P0685, P0686, P0687, P0689, or P0690 for the 2.0L engine or DTC P0685, P0686, P0687, P0689, or P0690 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0689 | Engine Controls Ignition Relay Feedback Circuit Low Voltage | ECM |

• | DTC P0685, P0689, or P0690 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0685, P0686, P0687, P0689, or P0690 for the 2.0L engine

• | DTC P0685, P0686, P0687, P0689, or P0690 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P068A | Engine Controls Ignition Relay De-Energized Too Early | ECM | DTC P068A or P068B
P068B | Engine Controls Ignition Relay De-Energized Too Late | ECM | DTC P068A or P068B
P0690 | Engine Controls Ignition Relay Feedback Circuit High Voltage | ECM |

• | DTC P0685, P0689, or P0690 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0685, P0686, P0687, P0689, or P0690 for the 2.0L engine

• | DTC P0685, P0686, P0687, P0689, or P0690 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P0691 | Cooling Fan Relay 1 Control Circuit Low Voltage | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694 for 4 cyl or V6 engines or DTC P0480-P0482 or P0691-P0696
P0692 | Cooling Fan Relay 1 Control Circuit High Voltage | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694 for 4 cyl or V6 engines or DTC P0480-P0482 or P0691-P0696
P0693 | Cooling Fan Relay 2 Control Circuit Low Voltage | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694 for 4 cyl or V6 engines or DTC P0480-P0482 or P0691-P0696
P0694 | Cooling Fan Relay 2 Control Circuit High Voltage | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694 for 4 cyl or V6 engines or DTC P0480-P0482 or P0691-P0696
P0695 | Cooling Fan Relay 3 Control Circuit Low Voltage | ECM | DTC P0480-P0482 or P0691-P0696
P0696 | Cooling Fan Relay 3 Control Circuit High Voltage | ECM | DTC P0480-P0482 or P0691-P0696
P0697 | 5-Volt Reference 3 Circuit | ECM |

• | DTC P0641, P0651, P0697, or P06A3 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0641-P0643, P0651-P0653, or P0697-P0699 for the 2.0L engine

• | DTC P0697 for the 2.0L (Diesel) engine

• | DTC P0641-P0643, P0651-P0653, or P0697-P0699 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P0698 | 5-Volt Reference 3 Circuit Low Voltage | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699 for the 2.0L engine or DTC P0641-P0643, P0651-P0653, or P0697-P0699 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0699 | 5-Volt Reference 3 Circuit High Voltage | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699 for the 2.0L engine or DTC P0641-P0643, P0651-P0653, or P0697-P0699 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P069E | Fuel Pump Flow Control Module Requested MIL Illumination | Fuel Pump Control Module | DTC P069E
P06A3 | 5-Volt Reference 4 Circuit | ECM | DTC P0641, P0651, P0697, or P06A3
P0700 | Transmission Control Module Requested MIL Illumination | ECM | DTC P0700 for the 2.0L engine or DTC P0700 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
TCM | DTC P0700
P0703 | Brake Switch Circuit 2 | ECM | DTC P0703
P0706 | Park/Neutral Position Switch Circuit | TCM | DTC P0706-P0708
P0707 | Park/Neutral Position Switch Circuit Low Voltage | TCM | DTC P0706-P0708
P0708 | Park/Neutral Position Switch Circuit High Voltage | TCM | DTC P0706-P0708
P0711 | Transmission Fluid Temperature Sensor Performance | TCM | DTC P0711, P0712, or P0713
P0712 | Transmission Fluid Temperature Sensor Circuit Low Voltage | TCM | DTC P0711, P0712, or P0713
P0713 | Transmission Fluid Temperature Sensor Circuit High Voltage | TCM | DTC P0711, P0712, or P0713
P0716 | Input Speed Sensor Performance | TCM | DTC P0716 or P0717
P0717 | Input Speed Sensor Circuit No Signal | TCM | DTC P0716 or P0717
P0721 | Output Speed Sensor Performance | TCM | DTC P0721 or P0722
P0722 | Output Speed Sensor Circuit No Signal | TCM | DTC P0721 or P0722
P0729 | 6th Gear Ratio Incorrect | TCM | DTC P0729
P0731 | 1st Gear Ratio Incorrect | TCM | DTC P0731
P0732 | 2nd Gear Ratio Incorrect | TCM | DTC P0732
P0733 | 3rd Gear Ratio Incorrect | TCM | DTC P0733
P0734 | 4th Gear Ratio Incorrect | TCM | DTC P0734
P0735 | 5th Gear Ratio Incorrect | TCM | DTC P0735
P0736 | Reverse Ratio Incorrect | TCM | DTC P0736
P0741 | Torque Converter Clutch System Stuck Off | TCM | DTC P0741 or P0742
P0742 | Torque Converter Clutch System Stuck On | TCM | DTC P0741 or P0742
P0748 | Line Pressure Control Solenoid Valve System Performance - Feedback Current Stuck | TCM | DTC P0748, P0961-P0963
P0778 | Pressure Control Solenoid Valve 1 System Performance - Feedback Current Stuck | TCM | DTC P0778, P0965-P0967
P0780 | Incorrect Shift Pattern | TCM | DTC P0780
P0798 | Pressure Control Solenoid Valve 2 System Performance - Feedback Current Stuck | TCM | DTC P0798, P0969-P0971
P0817 | Brake Transmission Shift Interlock Solenoid Actuator | TCM | DTC P0817
P0826 | Up and Down Shift Switch Circuit | TCM | DTC P0826
P0850 | Park/Neutral Position Switch Circuit | TCM | DTC P0850
P0856 | Traction Control Torque Request Circuit | ECM | DTC C0242 or P0856
P0961 | Line Pressure Control Solenoid Valve System Performance | TCM | DTC P0748, P0961-P0963
P0962 | Line Pressure Control Solenoid Valve Control Circuit Low Voltage | TCM | DTC P0748, P0961-P0963
P0963 | Line Pressure Control Solenoid Valve Contro Circuit High Voltage | TCM | DTC P0748, P0961-P0963
P0965 | Pressure Control Solenoid Valve 1 System Performance | TCM | DTC P0778, P0965-P0967
P0966 | Pressure Control Solenoid Valve 1 Control Circuit Low Voltage | TCM | DTC P0778, P0965-P0967
P0967 | Pressure Control Solenoid Valve 1 Control Circuit High Voltage | TCM | DTC P0778, P0965-P0967
P0969 | Pressure Control Solenoid Valve 2 System Performance | TCM | DTC P0798, P0969-P0971
P0970 | Pressure Control Solenoid Control Circuit Low Voltage | TCM | DTC P0798, P0969-P0971
P0971 | Pressure Control Solenoid Control Circuit High Voltage | TCM | DTC P0798, P0969-P0971
P0973 | Shift Solenoid Valve 2 Control Circuit Low Voltage | TCM | DTC P0973 or P0974
P0974 | Shift Solenoid Valve 2 Control Circuit High Voltage | TCM | DTC P0973 or P0974
P0985 | Shift Solenoid Valve 1 Control Circuit Low Voltage | TCM | DTC P0985 or P0986
P0986 | Shift Solenoid Valve 1 Control Circuit High Voltage | TCM | DTC P0985 or P0986
P1101 | Intake Air Flow System Performance | ECM | DTC P0068 or P1101
P1133 | HO2S Insufficient Switching Sensor 1 | ECM | DTC P0133, P0134, P013A, P013B, P013E, P013F, P0140, P1133, P2270, P2271, or P2A00
P1255 | Fuel Pump Flow Control Module Driver Over-temperature | Fuel Pump Control Module | DTC P1255 or P064A for the 2.0L engine or DTC P1255 or P064A for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P1409 | Exhaust Gas Recirculation Control Circuit | ECM | DTC P1409
P1484 | Cooling Fan System Performance | ECM | DTC P1484
P1516 | Throttle Actuator Control Motor Control Circuit | ECM | DTC P0133, P0134, P013A, P013B, P013E, P013F, P0140, P1133, P2270, P2271, or P2A00
P1551 | Throttle Valve Rest Position Not Reached During Learn | ECM | DTC P0638, P1551, P2100, P2101, P2119, or P2176 for the 2.0L engine or DTC P1551 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P160A | Vehicle Speed Limit Not Programmed | ECM | DTC P160A
P160D | Incorrect Engine Calibration Detected | ECM | DTC P160D for the 2.0L (Diesel) engine or DTC P0602, P0610, P0614, P0630, P160D, P160E, or P161F for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P160E | Engine Calibration Monitoring Not Programmed | ECM | DTC P160E for the 2.0L (Diesel) engine or DTC P0602, P0610, P0614, P0630, P160D, P160E, or P161F for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P161C | Tire Size Not Programmed | ECM | DTC P161C
P161F | Assembly Plant Mode Counter Not Programmed | ECM | DTC P0602, P0610, P0614, P0630, P160D, P160E, or P161F f
P1631 | Immobilizer Fuel Enable Signal Not Correct | ECM | DTC P1631
P1640 | Control Module Power Circuit Malfunction | ECM | DTC P1640
P1649 | Immobilizer Security Code Not Programmed | ECM | DTC P1649
P167A | Control Module HO2S 1 System Performance | ECM | DTC P0601-P0606, P062B, P064D, P167A, P167D, P2105, or P2610 for the 2.0L engine
P167D | Control Module Ignition Coil Internal Circuit | ECM | DTC P0601-P0606, P062B, P064D, P167A, P167D, P2105, or P2610 for the 2.0L engine or DTC P0603-P0606 or P167D for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P16F3 | Control Module Redundant Memory Performance | ECM | DTC P0601-P0604, P0606, P0607, P060D P062F, P16F3, or P2610
P1701 | Transmission Fluid Pressure Valve Position Switch Indicates Park/Neutral With Drive Ratio | TCM | DTC P1701
P1702 | Transmission Clutch 1 Stuck On - Engagement | TCM | DTC P1702-P1704
P1703 | Transmission Clutch 1 Stuck On - No Control | TCM | DTC P1702-P1704
P1704 | Transmission Clutch 1 - Slip Detected | TCM | DTC P1702-P1704
P1731 | 1st Gear Ratio Incorrect - with Engine Brake | TCM | DTC P1731
P1835 | Kickdown Switch Signal Performance - CAN Signal | TCM | DTC P1835
P1895 | Engine Torque Delivered Signal Message Counter Incorrect - CAN Signal | TCM | DTC P1895 or P1896
P1896 | Engine Control Module Driver Torque Request Signal Invalid Data - CAN Signal | TCM | DTC P1895 or P1896
P2008 | Intake Manifold Runner Control Valve Control Circuit Malfunction | ECM | DTC P2008
P2009 | Intake Manifold Runner Control Valve Control Circuit Low Voltage | ECM | DTC P2009 or P2010
P2010 | Intake Manifold Runner Control Valve Control Circuit High Voltage | ECM | DTC P2009 or P2010
P200A | Intake Manifold Runner Control Valve Control Circuit Performance | ECM | DTC P200A
P2015 | Intake Manifold Runner Control Valve Control Circuit Malfunction | ECM | DTC P2015
P2016 | Intake Manifold Runner Control Valve Control Circuit Malfunction | ECM | DTC P2016 or P2017
P2017 | Intake Manifold Runner Control Valve Control Circuit Malfunction | ECM | DTC P2016 or P2017
P2032 |  | ECM | DTC P2032 or P2033
P2033 |  | ECM | DTC P2032 or P2033
P2066 | Fuel Level Sensor 2 Performance | ECM | DTC P0461-P0463, P2066, P2067, or P2068
P2067 | Fuel Level Sensor 2 Circuit Low Voltage | ECM | DTC P0461-P0463, P2066, P2067, or P2068
P2068 | Fuel Level Sensor 2 Circuit High Voltage | ECM | DTC P0461-P0463, P2066, P2067, or P2068
P2088 | Intake Camshaft Position Actuator Solenoid Control Circuit Low Voltage | ECM | DTC P0010, P0013, or P2088-P2091 for the 2.0L engine
Intake Camshaft Position Actuator Solenoid Control Circuit Low Voltage Bank 1 | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P2089 | Intake Camshaft Position Actuator Solenoid Control Circuit High Voltage | ECM | DTC P0010, P0013, or P2088-P2091 for the 2.0L engine
Intake Camshaft Position Actuator Solenoid Control Circuit High Voltage Bank 1 | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P2090 | Exhaust Camshaft Position Actuator Solenoid Control Circuit Low Voltage | ECM | DTC P0010, P0013, or P2088-P2091 for the 2.0L engine
Exhaust Camshaft Position Actuator Solenoid Control Circuit Low Voltage Bank 1 | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P2091 | Exhaust Camshaft Position Actuator Solenoid Control Circuit High Voltage | ECM | DTC P0010, P0013, or P2088-P2091 for the 2.0L engine
Exhaust Camshaft Position Actuator Solenoid Control Circuit High Voltage Bank 1 | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P2092 | Intake Camshaft Position Actuator Solenoid Control Circuit Low Voltage Bank 2 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2093 | Intake Camshaft Position Actuator Solenoid Control Circuit High Voltage Bank 2 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2094 | Exhaust Camshaft Position Actuator Solenoid Control Circuit Low Voltage Bank 2 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2095 | Exhaust Camshaft Position Actuator Solenoid Control Circuit High Voltage Bank 2 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2096 | Post Catalyst Fuel Trim System Low Limit | ECM | DTC P2096
P2097 | Post Catalyst Fuel Trim System High Limit | ECM | DTC P2097
P2100 | Throttle Actuator Control Motor Control Circuit | ECM | DTC P0638, P1551, P2100, P2101, P2119, or P2176 for the 2.0L engine or DTC P0638, P2100-P2103, or P2119 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Intake Air Flow Valve Control Circuit Open | DTC P2100, P2102, P2103 for the 2.0L (Diesel) engine
P2101 | Control Module Throttle Actuator Position Performance | ECM |

• | DTC P0133, P0134, P013A, P013B, P013E, P013F, P0140, P1133, P2270, P2271, or P2A00 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0638, P1551, P2100, P2101, P2119, or P2176 for the 2.0L engine

• | DTC P0638, P2100-P2103, or P2119 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

Intake Air Flow Valve Control Circuit Malfunction | DTC P2101 for the 2.0L (Diesel) engine
P2102 | Throttle Actuator Control Motor Control Circuit Low Voltage | ECM | DTC P0638, P2100-P2103, or P2119 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Intake Air Flow Valve Control Circuit Short to Ground | DTC P2100, P2102, P2103 for the 2.0L (Diesel) engine
P2103 | Throttle Actuator Control Motor Control Circuit High Voltage | ECM | DTC P0638, P2100-P2103, or P2119 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Intake Air Flow Valve Control Circuit Short to Battery | DTC P2100, P2102, P2103 for the 2.0L (Diesel) engine
P2105 | Throttle Actuator Control System - Forced Engine Shut-down | ECM | DTC P0601-P0606, P062B, P064D, P167A, P167D, P2105, or P2610 for the 2.0L engine or DTC P2105 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P2119 | Throttle Closed Position Performance | ECM |

• | DTC P0133, P0134, P013A, P013B, P013E, P013F, P0140, P1133, P2270, P2271, or P2A00 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0638, P1551, P2100, P2101, P2119, or P2176 for the 2.0L engine

• | DTC P0638, P2100-P2103, or P2119 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P2120 | Accelerator Pedal Position Sensor 1 Circuit | ECM | DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138
P2122 | Accelerator Pedal Position Sensor 1 Circuit Low Voltage | ECM |

• | DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P2122 or P2123 for the 2.0L engine

• | DTC P2122, P2123, P2127, P2128, or P2138 for the 2.0L (Diesel) engine

• | DTC P2122, P2123, P2127, P2128, or P2138 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P2123 | Accelerator Pedal Position Sensor 1 Circuit High Voltage | ECM |

• | DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P2122 or P2123 for the 2.0L engine

• | DTC P2122, P2123, P2127, P2128, or P2138 for the 2.0L (Diesel) engine

• | DTC P2122, P2123, P2127, P2128, or P2138 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P2125 | Accelerator Pedal Position Sensor 2 Circuit | ECM | DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138
P2127 | Accelerator Pedal Position Sensor 2 Circuit Low Voltage | ECM |

• | DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P2127 or P2128 for the 2.0L engine

• | DTC P2122, P2123, P2127, P2128, or P2138 for the 2.0L (Diesel) engine

• | DTC P2122, P2123, P2127, P2128, or P2138 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P2128 | Accelerator Pedal Position Sensor 2 Circuit High Voltage | ECM |

• | DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P2127 or P2128 for the 2.0L engine

• | DTC P2122, P2123, P2127, P2128, or P2138 for the 2.0L (Diesel) engine

• | DTC P2122, P2123, P2127, P2128, or P2138 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P2135 | Throttle Position Sensors 1-2 Not Plausible | ECM | DTC P0120-P0123, P0220, P0222, P0223, or P2135
P2138 | Accelerator Pedal Position Sensors 1-2 Correlation | ECM | DTC P2127 or P2128 for the 2.0L engine or DTC P2122, P2123, P2127, P2128, or P2138 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Accelerator Pedal Position Sensors 1-2 Not Plausible | DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 1.6L (LDE) and 1.8L (2H0) engine or DTC P2122, P2123, P2127, P2128, or P2138 for the 2.0L (Diesel) engine
P2146 | Injector Positive Voltage Control Circuit Group 1 | ECM | DTC P0201-P0204, P0261, P0264, P0267, P0270, or P2146-P2157
P2147 | Injector Positive Voltage Control Circuit Group 1 Low Voltage | ECM | DTC P0201-P0204, P0261, P0264, P0267, P0270, or P2146-P2157
P2148 | Injector Positive Voltage Control Circuit Group 1 High Voltage | ECM | DTC P0201-P0204, P0261, P0264, P0267, P0270, or P2146-P2157
P2149 | Injector Positive Voltage Control Circuit Group 2 | ECM | DTC P0201-P0204, P0261, P0264, P0267, P0270, or P2146-P2157
P2150 | Injector Positive Voltage Control Circuit Group 2 Low Voltage | ECM | DTC P0201-P0204, P0261, P0264, P0267, P0270, or P2146-P2157
P2151 | Injector Positive Voltage Control Circuit Group 2 High Voltage | ECM | DTC P0201-P0204, P0261, P0264, P0267, P0270, or P2146-P2157
P2152 | Injector Positive Voltage Control Circuit Group 3 | ECM | DTC P0201-P0204, P0261, P0264, P0267, P0270, or P2146-P2157
P2153 | Injector Positive Voltage Control Circuit Group 3 Low Voltage | ECM | DTC P0201-P0204, P0261, P0264, P0267, P0270, or P2146-P2157
P2154 | Injector Positive Voltage Control Circuit Group 3 High Voltage | ECM | DTC P0201-P0204, P0261, P0264, P0267, P0270, or P2146-P2157
P2155 | Injector Positive Voltage Control Circuit Group 4 | ECM | DTC P0201-P0204, P0261, P0264, P0267, P0270, or P2146-P2157
P2156 | Injector Positive Voltage Control Circuit Group 4 Low Voltage | ECM | DTC P0201-P0204, P0261, P0264, P0267, P0270, or P2146-P2157
P2157 | Injector Positive Voltage Control Circuit Group 4 High Voltage | ECM | DTC P0201-P0204, P0261, P0264, P0267, P0270, or P2146-P2157
P2176 | Minimum Throttle Position Not Learned | ECM |

• | DTC P0133, P0134, P013A, P013B, P013E, P013F, P0140, P1133, P2270, P2271, or P2A00 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0638, P1551, P2100, P2101, P2119, or P2176 for the 2.0L engine

• | DTC P2176 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P2177 | Fuel Trim System Lean at Cruise or Accel | ECM | DTC P2177 or P2187 for the 2.0L engine or DTC P2177 or P2187 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P2178 | Fuel Trim System Rich at Cruise or Accel | ECM | DTC P2178 or P2188 for the 2.0L engine or DTC P2178 or P2188 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P2181 |  | ECM | DTC P2181
P2187 | Fuel Trim System Lean at Idle | ECM | DTC P2177 or P2187 for the 2.0L engine or DTC P2177 or P2187 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P2188 | Fuel Trim System Rich at Idle | ECM | DTC P2178 or P2188 for the 2.0L engine or DTC P2178 or P2188 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P2195 | HO2S Signal Biased Lean Sensor 1 | ECM | DTC P0130, P0131, P0132, P0133, P2195, P2196, P2231, or P2297
P2196 | HO2S Signal Biased Rich Sensor 1 | ECM | DTC P0130, P0131, P0132, P0133, P2195, P2196, P2231, or P2297
P2199 | Intake Air Temperature Sensor 1-2 Correlation | ECM | DTC P0130, P0131, P0132, P0133, P2195, P2196, P2231, or P2297
P2227 | Barometric Pressure Sensor Performance | ECM | DTC P2227, P2228, or P2229 for the 2.0L engine or DTC P2227, P2228, or P2229 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P2228 | Barometric Pressure Sensor Circuit Low Voltage | ECM |

• | DTC P2227, P2228, or P2229 for the 2.0L engine

• | DTC P2228 or P2229 for the 2.0L (Diesel) engine

• | DTC P2227, P2228, or P2229 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P2229 | Barometric Pressure Sensor Circuit High Voltage | ECM |

• | DTC P2227, P2228, or P2229 for the 2.0L engine

• | DTC P2228 or P2229 for the 2.0L (Diesel) engine

• | DTC P2227, P2228, or P2229 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P2231 | HO2S Signal Circuit Shorted to Heater Circuit Sensor 1 | ECM | DTC P0130, P0131, P0132, P0133, P2195, P2196, P2231, or P2297 for the 2.0L engine or DTC P2231 for the 2.0L (Diesel) engine
P2232 | HO2S Signal Circuit Shorted to Heater Circuit Sensor 2 | ECM | DTC P0137, P0138, P0140, P2232, P2270, or P2271 for the 2.0L engine or DTC P2232 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P2237 | HO2S Pumping Current Control Circuit Sensor 1 | ECM | DTC P0137, P0138, P0140, P2232, P2270, or P2271
P2238 | HO2S Pump Current Control Circuit Low Voltage Sensor 1 | ECM | DTC P0137, P0138, P0140, P2232, P2270, or P2271
P2239 | HO2S Pump Current Control Circuit High Voltage Sensor 1 | ECM | DTC P0137, P0138, P0140, P2232, P2270, or P2271
P2243 | HO2S Reference Voltage Circuit Sensor 1 | ECM | DTC P0137, P0138, P0140, P2232, P2270, or P2271 for the 2.0L engine or DTC P2243 for the 2.0L (Diesel) engine
P2251 | HO2S Low Reference Circuit Sensor 1 | ECM | DTC P0137, P0138, P0140, P2232, P2270, or P2271
P2261 | Turbocharger Bypass Valve Stuck Closed | ECM | DTC P2261 for the 2.0L engine or DTC P2261 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P2263 | Turbocharger Boost System Performance | ECM | DTC P2263
P2265 | Water in Fuel Sensor Circuit | ECM | DTC P2265
P2270 | HO2S Signal Stuck Lean Sensor 2 | ECM |

• | DTC P0133, P0134, P013A, P013B, P013E, P013F, P0140, P1133, P2270, P2271, or P2A00 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0137, P0138, P0140, P2232, P2270, or P2271 for the 2.0L engine

• | DTC P2270 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P2271 | HO2S Signal Stuck Rich Sensor 2 | ECM |

• | DTC P0133, P0134, P013A, P013B, P013E, P013F, P0140, P1133, P2270, P2271, or P2A00 for the 1.6L (LDE) and 1.8L (2H0) engine

• | DTC P0137, P0138, P0140, P2232, P2270, or P2271 for the 2.0L engine

• | DTC P2271 for the 2.8L, 3.0L, 3.2L, or 3.6L engine

P2282 | Mass Air Flow Sensor Performance | ECM | DTC P2282
P2297 | HO2S Performance During Decel Fuel Cut-Off Sensor 1 | ECM | DTC P0130, P0131, P0132, P0133, P2195, P2196, P2231, or P2297
P2300 | Ignition Coil 1 Control Circuit Low Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, or P2310 for the 2.0L engine or DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P2301 | Ignition Coil 1 Control Circuit High Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, or P2310 for the 2.0L engine or DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P2303 | Ignition Coil 2 Control Circuit Low Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, or P2310 for the 2.0L engine or DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P2304 | Ignition Coil 2 Control Circuit High Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, or P2310 for the 2.0L engine or DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P2306 | Ignition Coil 3 Control Circuit Low Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, or P2310 for the 2.0L engine or DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P2307 | Ignition Coil 3 Control Circuit High Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, or P2310 for the 2.0L engine or DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P2309 | Ignition Coil 4 Control Circuit Low Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, or P2310 for the 2.0L engine or DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P2310 | Ignition Coil 4 Control Circuit High Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, or P2310 for the 2.0L engine or DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P2312 | Ignition Coil 5 Control Circuit Low Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2313 | Ignition Coil 5 Control Circuit High Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2315 | Ignition Coil 6 Control Circuit Low Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2316 | Ignition Coil 6 Control Circuit High Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2413 | Exhaust Gas Recirculation (EGR) System Performance | ECM | DTC P2413
P2431 | Secondary Air Injection System Pressure Sensor Performance | ECM | DTC P2431-P2433
P2432 | Secondary Air Injection System Pressure Sensor Circuit Low Voltage | ECM | DTC P2431-P2433
P2433 | Secondary Air Injection System Pressure Sensor Circuit High Voltage | ECM | DTC P2431-P2433
P2444 | Secondary Air Injection System Pump Stuck On | ECM | DTC P0418, P2444, or P2445
P2445 | Secondary Air Injection System Pump Stuck Off | ECM | DTC P0418, P2444, or P2445
P2453 | Diesel Particulate Filter Differential Pressure Sensor Performance | ECM | DTC P2453
P2454 | Diesel Particulate Filter Differential Pressure Sensor Circuit Low Voltage | ECM | DTC P2454 or P2455
P2455 | Diesel Particulate Filter Differential Pressure Sensor Circuit High Voltage | ECM | DTC P2454 or P2455
P2458 | Diesel Particulate Filter Regeneration Time | ECM | DTC P2458
P2459 | Diesel Particulate Filter Regeneration Frequency | ECM | DTC P2459
P245A | Exhaust Gas Recirculation Cooler Bypass Control Circuit | ECM | DTC P245A-P245D
P245B | Exhaust Gas Recirculation Cooler Bypass Solenoid Valve Control Circuit Malfunction | ECM | DTC P245A-P245D
P245C | Exhaust Gas Recirculation Cooler Bypass Solenoid Valve Control Circuit Short to Ground | ECM | DTC P245A-P245D
P245D | Exhaust Gas Recirculation Cooler Bypass Solenoid Valve Control Circuit Short to Battery | ECM | DTC P245A-P245D
P2534 | Ignition 1 Switch Circuit Low Voltage | ECM | DTC P2534 for the 2.0L engine or DTC P2534 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P2564 | Turbocharger Boost Control Position Sensor Circuit Low Voltage | ECM | DTC P2564 or P2565
P2565 | Turbocharger Boost Control Position Sensor Circuit High Voltage | ECM | DTC P2564 or P2565
P2610 | Control Module Ignition Off Timer Performance | ECM | DTC P0601-P0604, P0606, P0607, P060D P062F, P16F3, or P2610 for the 1.6L (LDE) and 1.8L (2H0) engine or DTC P0601-P0606, P062B, P064D, P167A, P167D, P2105, or P2610 for the 2.0L engine
P2617 | Crankshaft Position Signal Output Circuit | ECM | DTC P2617
P2626 | HO2S Pumping Current Trim Circuit Sensor 1 | ECM | DTC P0137, P0138, P0140, P2232, P2270, or P2271 for the 2.0L engine or DTC P2626 for the 2.0L (Diesel) engine
P2635 | Fuel Pump Flow Performance | Fuel Pump Control Module | DTC P2635 for the 2.0L engine or DTC P2635 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P2687 | Fuel Heater Relay Control Circuit | ECM | DTC P2687-P2689
P2688 | Fuel Heater Relay Control Circuit Low Voltage | ECM | DTC P2687-P2689
P2689 | Fuel Heater Relay Control Circuit High Voltage | ECM | DTC P2687-P2689
P268C | Cylinder 1 Injector Calibration Incorrect | ECM | DTC P268C-P268F
P268D | Cylinder 2 Injector Calibration Incorrect | ECM | DTC P268C-P268F
P268E | Cylinder 3 Injector Calibration Incorrect | ECM | DTC P268C-P268F
P268F | Cylinder 4 Injector Calibration Incorrect | ECM | DTC P268C-P268F
P2716 | Pressure Control Solenoid Valve 3 System Performance | TCM | DTC P2716 or P2719-P2721
P2719 | Pressure Control Solenoid Valve 3 System Performance | TCM | DTC P2716 or P2719-P2721
P2720 | Pressure Control Solenoid Valve 3 Control Circuit Low Voltage | TCM | DTC P2716 or P2719-P2721
P2721 | Pressure Control Solenoid Valve 3 Control Circuit High Voltage | TCM | DTC P2716 or P2719-P2721
P2725 | Brake Band Pressure Control Solenoid Valve Control Circuit | TCM | DTC P2725, P2728, P2729, or P2830
P2728 | Brake Band Pressure Control Solenoid Valve Performance | TCM | DTC P2725, P2728, P2729, or P2830
P2729 | Brake Band Pressure Control Solenoid Valve Control Circuit Low Voltage | TCM | DTC P2725, P2728, P2729, or P2830
P2730 | Brake Band Pressure Control Solenoid Valve Control Circuit High Voltage | TCM | DTC P2725, P2728, P2729, or P2830
P2759 | Brake Band Pressure Control Solenoid Valve Control Circuit | TCM | DTC P2759 or P2762-P2764
P2762 | Brake Band Pressure Control Solenoid Valve Performance | TCM | DTC P2759 or P2762-P2764
P2763 | Brake Band Pressure Control Solenoid Valve Control Circuit Low Voltage | TCM | DTC P2759 or P2762-P2764
P2764 | Brake Band Pressure Control Solenoid Valve Control Circuit High Voltage | TCM | DTC P2759 or P2762-P2764
P2A00 | HO2S Circuit Closed Loop Performance Sensor 1 | ECM | DTC P0133, P0134, P013A, P013B, P013E, P013F, P0140, P1133, P2270, P2271, or P2A00 for the 1.6L (LDE) and 1.8L (2H0) engine or DTC P2A00 for the 2.0L (Diesel) engine
U0001 | High Speed Controller Area Network Communication Bus | -- | DTC U0001
U0002 | High Speed Controller Area Network Communication Bus | -- | DTC U0002
U0020 | Low Speed Controller Area Network Communication Bus Performance | -- | DTC U0020
U0073 | Control Module Communication Bus Off | -- | DTC U0073 or U2100
U0074 | Control Module Communication Bus B Off | -- | DTC U0074
U0100 - U0299 | Lost Communication With XXX Control Module | -- | DTC U0100-U0299
U0301 | Software Incompatibility with Engine Control Module | -- | DTC U0300-U0336
U0315 | Software Incompatibility with Electronic Brake Control Module | -- | DTC U0300-U0336
U0400 - U05FF | Invalid Data Received | -- | DTC U0400-U05FF
U1500 - U15BF | Inter-device Dedicated Bus | -- | DTC U1500-U15BF
U1814 | Powertrain Wake Up Communication Circuit | BCM | DTC U1814
U18B9 | Primary High Speed Controller Area Network Bus Subnet Configuration List | -- | DTC U18B9-U18BF
U18BF | Secondary High Speed Controller Area Network Bus Subnet Configuration List | -- | DTC U18B9-U18BF
U2099 | High Speed Communication Enable Circuit | BCM | DTC U2099
U2100 | Controller Area Network Bus Communication | -- | DTC U0073 or U2100
U2101 | Controller Area Network Bus Maximum Configuration List | -- | DTC U2101
U2103 | Fewer Controllers On Bus Than Programmed | -- | DTC U2103
U2105 - U2199 | Lost Communication With XXX Control Module | -- | DTC U2105-U2199