For 1990-2009 cars

## Engine Oil Cooler Housing Removal LLU

1. Remove the 2 engine oil cooler pipe bolts (1).
2. Remove the engine oil cooler pipe (2).
3. Remove the 5 engine oil cooler housing bolts (2).
4. Remove the engine oil cooler housing (1).
5. Remove the engine oil cooler inlet pipe (3).

## Engine Oil Cooler Housing Removal LDE, 2H0

1. Remove the 2 engine oil cooler pipe bolts (1)
2. Remove the oil cooler pipe (2)
3. Remove the 5 oil filter housing bolts (2).
4. Remove the oil filter housing (1).
5. Remove the engine oil cooler inlet pipe (3).