For 1990-2009 cars

## Oil Level Indicator and Tube Installation LDK

1. Lubricate the oil level indicator tube O-ring, refer to Adhesives, Fluids, Lubricants, and Sealers.
2. Install the oil level indicator (2) and the oil level indicator tube (1) into the oil pan.
3. Install the oil level indicator tube bracket to the intake manifold.

Caution: Refer to Fastener Caution in the Preface section.

4. Install the oil level indicator tube bracket bolt and tighten to 10 N·m (89 lb in).
5. Install the electrical wiring harness to the oil level indicator tube.
6. Install the knock sensor wiring clip into the oil level indicator tube.