For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the power brake booster vacuum sensor from the air cleaner housing.
2. Disconnect the mass airflow sensor wiring harness connector.

1 | Secondary Air Injection Pipe Quick Connect Fitting
2 | Air Cleaner Outlet Duct Fastener Caution: Refer to Fastener Caution in the Preface section. Tighten 3.5 N·m (31 lb in)
3 | Air Cleaner Outlet Duct
4 | Air Cleaner Housing Fastener (Qty: 6) Tighten 3 N·m (27 lb in)
5 | Air Cleaner Upper Housing
6 | Air Cleaner Element