For 1990-2009 cars

## Radiator Outlet Hose Replacement LDE/A16XER, 2HO/A18XER

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Drain the cooling system. Refer to Cooling System Draining and Filling
2. Remove the air cleaner outlet duct. Refer to LINK.

1 | Radiator Inlet Hose

#### Procedure

1. Detach the quick release hose connector from the radiator.
2. After installation, fill the coolant reservoir to the fill level. Refer to Cooling System Draining and Filling
3. Inspect cooling system for leaks.

2 | Radiator Inlet Hose

#### Procedure

Using a hose clamp tool reposition the radiator inlet hose clamp and detach from the engine.

3 | Coolant Cross Over Pipe

#### Procedure

1. Release the coolant hose from the top of the fan shroud.
2. Release the coolant hose from the charge air cooler pipes.
3. Detach the coolant hose from the radiator surge tank.

4 | Radiator Outlet Hose

#### Procedure

1. After installation, Fill the coolant reservoir to the fill level. Refer to Cooling System Draining and Filling
2. Inspect cooling system for leaks.

## Radiator Outlet Hose Replacement LDK/A20NHT

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove engine appearance cover replacement. Refer to LINK.
2. Draing the cooling system. Refer to Cooling System Draining and Filling.

1 | Radiator Outlet Hose Replacement Clamp (Qty: 3 )