For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: Refer to Brake Dust Warning in the Preface section.

#### Preliminary Procedure

1. Remove the brake caliper. Refer to Rear Brake Caliper Replacement.
2. Remove the brake pads. Refer to Rear Disc Brake Pads Replacement.

1 | Bracket Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Apply suitable locking agent on the bolts. Refer to Adhesives, Fluids, Lubricants, and Sealers.

Tighten
163 N·m (120 lb ft)

2 | Rear Brake Caliper Bracket