For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the roof console reading lamp bezel. Refer to Roof Console Reading Lamp Bezel Replacement.
2. Perform the Sunroof Motor/Actuator Initialization/teach process.

1 | Sunroof Sunshade Motor Control Fastener (Qty: 3) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

1. Turn the ignition OFF.
2. Disconnect the electrical connectors.
3. Remove the sunroof sunshade motor control fasteners.
4. Remove the sunroof sunshade motor.

Tighten
4 N·m (35 lb in)

2 | Sunroof Sunshade Motor