For 1990-2009 cars

## Liftgate Wiring Harness Replacement Left Side

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Open Liftgate.
2. Remove the Liftgate Window Side Garnish Molding. Refer to Liftgate Window Side Garnish Molding Replacement.
3. Remove the liftgate trim finish panel. Refer to XXXXX.

1 | Liftgate Wiring Harness Retainer (Qty: 12)

#### Procedure

Disconnect the electrical connector.

2 | Liftgate Wiring Harness

## Liftgate Wiring Harness Replacement Right Side

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Open Liftgate.
2. Remove the Liftgate Window Side Garnish Molding. Refer to Liftgate Window Side Garnish Molding Replacement
3. Remove the liftgate trim finish panel. Refer to XXXXX.

1 | Liftgate Wiring Harness Retainer (Qty: 12)

#### Procedure

Disconnect the electrical connector.

2 | Liftgate Wiring Harness