For 1990-2009 cars

## Engine Flywheel Installation LLU

#### Special Tools

• | EN-652 Flywheel Holder

• | EN-45059 Torque Angle Sensor Kit

For equivalent regional tools, refer to Special Tools.

1. Clean the thread in the crankshaft.
2. Install the flywheel (2).
3. Install the EN-652 holder (1).

Caution: Refer to Fastener Caution in the Preface section.

4. Install the 6 NEW flywheel bolts (1, 2) and tighten the bolts in 3 passes using the EN-45059 sensor kit :

• | First pass to 35 N·m (26 lb ft).

• | Second pass to additional 30 degrees.

• | Third pass to an additional 15 degrees.

5. Remove the EN-652 holder .