For 1990-2009 cars

1. Install the NEW 12 fuel injector seals (3).
2. Install the 6 fuel injectors (2).
3. Install the 6 fuel injector retainer clips (1).
4. Install the fuel injector rail (2).

Caution: Refer to Fastener Caution in the Preface section.

5. Install the 3 fuel injector rail bolts (1) and tighten to 10 N·m (89 lb in).
6. Install the fuel injector wiring harness (2).
7. Install the 6 fuel injector wiring harness plug (1).