For 1990-2009 cars

## Duct Air Temperature Sensor Replacement - Lower Right Side Left Hand Drive with CJ2

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove instrument panel compartment. Refer to Instrument Panel Compartment Replacement.
2. Remove the floor air outlet duct - right side. Refer to Floor Air Outlet Duct Replacement - Right Side.

1 | Air Temperature Sensor Replacement - Lower Right Side

#### Procedure

1. Disconnect the air temperature sensor electrical connector.
2. Twist and pull the lower air temperature sensor from the HVAC module assembly.