For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement.

1 | Headlamp Fastener (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m(22 lb in)
2 | Headlamp

#### Procedure

1. Pull up and forward in order to release the headlamp.
2. Pull the headlamp assembly forward far enough to access the electrical connection.
3. Disconnect the electrical connections.
4. Remove the headlamp assembly.
5. Aim the headlamps after installation. Refer to Headlamp Aiming.