For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove engine appearance cover replacement. Refer to XXX.
2. Raise the vehicle by its full height. Refer to Lifting and Jacking the Vehicle.
3. Drain the cooling system. Refer to Cooling System Draining and Filling.
4. Remove the turbocharger brace. Refer to XXX.

1 | Turbocharger Coolant Return Pipe Fastener (Qty: 2) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Use a new gasket.

Tighten
X N·m (X lb in)

2 | Turbocharger Coolant Return Pipe