For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. SIR Disabling and Enabling. Refer to SIR Disabling and Enabling.
2. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.

1 | Cap
2 | Driver or Passenger Seat Belt Fastener Caution: Refer to Fastener Caution in the Preface section. Tighten 5 N·m (44 lb in)
3 | Seat Belt Tensioner Cover
4 | Driver or Passenger Seat Belt
5 | Driver or Passenger Seat Fastener (Qty: 2)

#### Procedure

1. Move front seat high adjuster in middle position.
2. Disconnect the battery.
3. Seat belt release at seat belt tensioner.
4. Disconnect the central wiring harness connector at bottom.
5. Unscrew both fasteners at the rail guide.
6. Remove the front seat out of the vehicle with two persons.

Tighten
20 N·m (15 lb ft)

6 | Driver or Passenger Seat