For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat. Refer to Rear Seat Replacement.
2. Remove rear seat back-left side. Refer to LINK.
3. Remove rear seat head restraint. Refer to Rear Seat Head Restraint Replacement.
4. Remove the rear seat center head restraint. Refer to Rear Seat Center Head Restraint Installation.
5. Remove the rear seat head restraint guides. Refer to Rear Seat Head Restraint Guide Replacement.
6. Remove the rear seat back cushion latch release knob bezel. Refer to Rear Seat Back Cushion Latch Release Knob Bezel Replacement.
7. Remove rear seat back cushion cover and pad. Refer to Rear Seat Back Cushion Cover and Pad Replacement - Left Side.

1 | Rear Seat Back Cushion Latch Fastener (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 45 N·m (33 lb ft)