For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Rear Side Door Check Link Fastener Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

1. Disconnect the door electrical connector.
2. Support the door before removing the hinge fastener.
3. With the aid of an assistant, remove the door.

Tighten
22 N·m (16.2 lb ft)

2 | Rear Side Door Hinge Fastener to Hinge Tighten 25 N·m (18.4 lb ft)
3 | Rear Side Door Hinge Fastener to Door (Qty: 2) Tighten 25 N·m (18.4 lb ft)
4 | Rear Side Door Assembly

#### Procedure

When replacing the door it is necessary to transfer all of the internal components.