For 1990-2009 cars

#### Special Tools

• | EN-45000 Remover

• | EN-47635 Installer

• | EN-41998-B Installer

For equivalent regional tools, refer to Special Tools.

### Removal Procedure

1. Remove the crankshaft balancer. Refer to Crankshaft Balancer Replacement.
2. Remove the crankshaft front oil seal (1) with EN-45000 remover (2).

### Installation Procedure

Important: Do not lubricate the crankshaft front oil seal or the crankshaft balancer sealing surfaces.

1. Place the crankshaft front oil seal (1) on EN-47635 installer (2) and insert evenly in engine front cover.
2. Install EN-41998-B installer (3, 4) into the crankshaft.
3. Screw the nut (3) in until the crankshaft front oil seal is in full contact.
4. Remove EN-41998-B installer and EN-47635 installer .
5. Install the crankshaft balancer. Refer to Crankshaft Balancer Replacement.