For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Release the charge air cooler outlet pipe. Refer to LINK.

1 | Throttle Body Assembly Fastener (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in)
2 | Throttle Body

#### Procedure

Disconnect the electrical connector.