For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the instrument panel (I/P) assembly. Refer to Instrument Panel Assembly Replacement
2. Remove both front and rear side door still trim plates. Refer to Front and Rear Side Door Sill Trim Plate Replacement
3. Remove the Steering Column. Refer to Steering Column Replacement
4. Remove the body control module bracket. Refer to Body Control Module Replacement

1 | Instrument Panel Tie Bar Assembly Fastener (Qty: 10) Caution: Refer to Fastener Caution in the Preface section. Tighten 22 N·m (16 lb ft)
2 | Heater and Air Conditioning Evaporator and Blower Module Fastener (Qty: 3)

#### Procedure

Release the Heater and Air Conditioning Evaporator and Blower Module from the I/P Tie Bar and secure the module at the Body.

Tighten
5 N·m (44 lb in)

3 | Instrument Panel Tie Bar Assembly

#### Procedures

1. Remove the hood release handle.
2. Note location and routing of the I/P wiring harness prior to removal of the I/P Tie Bar assembly to ensure proper reinstallation.
3. Disconnect the wiring harness from the I/P Tie Bar assembly.
4. With the aid of an assistant, remove the I/P Tie Bar assembly from the vehicle.
5. If replacing the I/P Tie Bar assembly, transfer all necessary components.