For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement.
2. Remove the headlamp washer nozzle hole cover. Refer to Headlamp Washer Nozzle Hole Cover Replacement.

1 | Headlamp Washer Nozzle Actuator Tip Use a small flat-bladed tool to release the headlamp washer nozzle actuator bracket locking retainer from the headlamp washer nozzle actuator.