For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the steering wheel. Refer to Steering Wheel Replacement.
2. Loosen the steering column trim covers for access. Refer to Steering Column Trim Cover Replacement.

1 | Inflatable Restraint Steering Wheel Module Coil Bolt (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 15 N·m (11 lb ft)
2 | Inflatable Restraint Steering Wheel Module Coil

#### Procedure

1. Disconnect any electrical connectors as needed.
2. Transfer the steering wheel position sensor. Refer to Steering Wheel Position Sensor Replacement.

Tip

• | Do not remove the centering tab from a new inflatable restraint steering wheel module coil until it has been installed or re-centering will be required.

• | If re-centering of the inflatable restraint steering wheel module coil is needed then refer to Inflatable Restraint Steering Wheel Module Coil Centering.