For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: Refer to Brake Fluid Irritant Warning in the Preface section. Warning: Refer to Brake Dust Warning in the Preface section.

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the tire and wheel. Refer to Tire and Wheel Removal and Installation.

1 | Brake Pipe Fitting Caution: Refer to Fastener Caution in the Preface section. Tip

• | Cap the brake pipe fitting to prevent brake fluid loss and contamination.

• | Use a flare nut wrench on the brake pipe fitting and a backup wrench on the brake hose.

Tighten
18 N·m(13 lb ft)

2 | Brake Hose Retainer
3 | Brake Hose Fitting Bolt Tighten 40 N·m(30 lb ft)
4 | Brake Hose Fitting Gasket (Qty: 2)

#### Procedure

Install NEW gaskets. DO NOT reuse the brake hose fitting gaskets.

5 | Rear Brake Hose

#### Procedure

Bleed the hydraulic brake system. Refer to Hydraulic Brake System Bleeding.