For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the instrument panel molding - passenger side. Refer to Instrument Panel Molding Replacement - Passenger Side.
2. Remove the instrument panel molding - driver side. Refer to Instrument Panel Molding Replacement - Driver Side.

1 | Instrument Panel Lower and Upper Center Trim Panel Fastener (Qty: 6)

#### Procedure

1. Release both center trim panels from the instrument panel and separate the parts.
2. Use a flat-bladed plastic trim tool in order to release the retaining clips securing the upper center trim panel to the instrument panel.
3. Disconnect the electrical connections.

2 | Instrument Panel Lower Center Trim Panel Retainer (Qty: 2)

#### Procedure

Release the lower center trim panel from the upper center trim panel.

3 | Instrument Panel Lower Center Trim Panel Tip When replacing the lower center trim panel, transfer parts as necessary.