For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the front and rear side door sill trim plate. Refer to Front and Rear Side Door Sill Trim Plate Replacement.
2. Move seat to full forward position.

1 | Center Pillar Lower Trim Panel Retainer (Qty 3)

#### Procedure

1. Remove the center pillar trim panel.
2. Release the retainer on the rear side of the center pillar upper trim panel.

2 | Center Pillar Lower Trim Panel