For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the front side door trim panel. Refer to Front Side Door Trim Panel Replacement
2. Remove the front side door window outer sealing strip. Refer to Front Side Door Window Outer Sealing Strip Replacement
3. Remove the rear side door window frame garnish molding. Refer to Front Side Door Window Frame Garnish Molding Replacement

1 | Front Side Door Window Weatherstrip Retainer
2 | Front Side Door Window Weatherstrip

#### Procedure

Pull the front side door window weatherstrip from the window frame to remove.