For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove engine appearance cover replacement. Refer to XXX.

1 | Charge Air Bypass Valve Vacuum Tank

#### Procedure

Release the vacuum hose from charger air bypass valve vacuum tank.

2 | Charge Air Bypass Valve Vacuum Tank Fastener (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten X N·m (X lb ft)
3 | Charge Air Bypass Valve Vacuum Tank