For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear compartment side trim panel. Refer to Rear Compartment Side Trim Panel Replacement

Caution: When a hood hold open device is being removed or installed, provide alternate support to avoid the possibility of damage to the vehicle or personal injury.

Notice: Apply pressure only at the end of the liftgate/hood assist rod that you are removing or attaching. Do NOT apply pressure to the middle of the rod because damage or bending will result.

1 | Rear Compartment Lid Strut Retainer (Qty: 2)

#### Procedure

1. Release the locking tabs on the strut.
2. Ensure the clip is fully seated when the rod is reinstalled. If the clip cannot be fully seated a new rod should be installed.