For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Front Seat Adjuster Track Finish Cover Fastener Caution: Refer to Fastener Caution in the Preface section. Tighten 3.5 N·m (31 lb in)
2 | Front Seat Adjuster Track Finish Cover

#### Procedure

1. Move front seat height adjuster into the middle position.
2. Move the driver or passenger seat fully forward.
3. Clip out the front seat adjuster track finish cover at rear.
4. Move the front seat adjuster track finish cover at front.
5. Remove the front seat adjuster track finish cover.