For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you review the Steering Wheel and Column Description and Operation and perform the necessary inspections? | Go to Step 2 | Go to Steering Wheel and Column Description and Operation
2 | Verify that the steering column is loose. Is the steering column loose? | Go to Step 3 | System OK
3 | Inspect the steering column mounting features for the following conditions.

• | Steering column mounting fasteners for looseness

• | Steering column mounting features are sheared

Are the steering column mounting features loose?

Go to Step 5

Go to Step 4

4 | Inspect the upper and/or lower bearings for looseness. Are any of the bearings worn or loose? | Go to Step 6 | Go to Step 7
5 | Note: If the steering column mounting feature is damaged or sheared, the steering column will need to be replaced. Refer to Steering Column Replacement. Tighten the steering column mounting fastener to specifications. Refer to Fastener Tightening Specifications.

Did you complete the repair?

Go to Step 7

--

6 | Note: If the steering column upper and/or lower bearings are not serviceable, the steering column will need to be replaced. Refer to Steering Column Replacement. Replace the upper and/or lower bearings, if serviceable. Did you complete the repair? | Go to Step 7 | --
7 | Operate the steering column in order to verify the repair. Did you correct the condition? | System OK | Go to Step 3