For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Position the window approximately half way down in the door.
2. Remove the rear side door window rear channel. Refer to Rear Side Door Window Rear Channel Replacement

1 | Rear Side Door Window to Regulator Retainer

#### Procedure

1. Access the retainer pin through the hole in the window regulator.
2. Use a suitable tool to drive the center pin out of the outer retainer.
3. Use a suitable tool to drive the pin out of the window.

2 | Rear Side Door Window Regulator Sash Tip Raise the window up out of the sash.
3 | Rear Side Door Window

#### Procedure

1. Lower the window into the door until it is free from the front and rear run channel.
2. Rotate the rear door window as necessary to remove it from the door.